<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<packages>
<package name="DIL40">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="PLCC44">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="S44">
<description>&lt;b&gt;PLCC SOCKET&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO20L">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; large</description>
</package>
<package name="DIL22-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="LCC20">
<description>&lt;b&gt;Leadless Chip Carrier&lt;/b&gt;&lt;p&gt; Ceramic Package</description>
</package>
<package name="DIL24-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
<package name="SO20W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL22">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOCKET-16">
<description>&lt;b&gt;Dual In Line Socket&lt;/b&gt;</description>
</package>
<package name="SOCKET-14">
<description>&lt;b&gt;Dual In Line Socket&lt;/b&gt;</description>
</package>
<package name="7110">
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="D_R-PDSO-G8">
<description>&lt;b&gt;D (R-PDSO-G8)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/slos063b/slos063b.pdf</description>
</package>
<package name="PS_R-PDSO-G8">
<description>&lt;b&gt;PS (R-PDSO-G8)&lt;/b&gt;&lt;p&gt;
Source: www.ti.com sn75452b.pdf</description>
</package>
<package name="SOIC127P1032X265-20N">
</package>
<package name="SOIC127P1030X265-20N">
</package>
<package name="DIP254P762X508-20">
</package>
<package name="SOIC127P1030X265-24N">
</package>
<package name="24HP">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
horizontal with mounting pad</description>
</package>
<package name="GPIB-PINHD-2X12">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="GPIB-PINHD-2X12/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="RASPBERRY-PI-PLUS-CAM_NOTCH">
<description>For use with TOBY :

REF-182684-02 2x20 SIF 10.00mm length PCB tails 
REF-182665-01 2x20 pos. with PCB alignment peg option 
REF-182683-02  2x20 SIF 4.93mm length PCB tails 

http://www.toby.co.uk/content/catalogue/products.aspx?series=REF-18xxxx-0x
http://www.toby.co.uk/content/catalogue/products.aspx?series=REF-1826xx-0x
http://www.toby.co.uk/content/catalogue/products.aspx?series=REF-18xxxx-0x</description>
</package>
<package name="RASPBERRY-PI-PLUS">
</package>
<package name="RASPBERRY-PI-PLUS-DISPLAY/CAM_NOTCH">
</package>
<package name="RASPBERRY-PI-PLUS-NOOUTLINE">
</package>
<package name="RASPBERRY-PI-PLUS-HEADERONLY">
</package>
<package name="RASPBERRY-PI-ZERO">
</package>
<package name="RASPBERRY-PI-ZERO-REFLOWHEADER">
</package>
<package name="2X20">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="DIL28">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="RN-8">
<description>&lt;b&gt;RESISTOR NETWORK&lt;/b&gt;</description>
</package>
<package name="2X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X05/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X12">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X12/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X17">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X17/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X10/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="DIP254P762X508-16">
</package>
<package name="DIL08S">
<description>&lt;b&gt;CRYSTAL RESONATOR&lt;/b&gt;</description>
</package>
<package name="DIL14S">
<description>&lt;b&gt;CRYSTAL RESONATOR&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="8087">
<pin name="A19/S6"/>
<pin name="A18/S5"/>
<pin name="A17/S4"/>
<pin name="A16/S3"/>
<pin name="AD15"/>
<pin name="AD14"/>
<pin name="AD13"/>
<pin name="AD12"/>
<pin name="AD11"/>
<pin name="AD10"/>
<pin name="AD9"/>
<pin name="AD8"/>
<pin name="AD7"/>
<pin name="AD6"/>
<pin name="AD5"/>
<pin name="AD4"/>
<pin name="AD3"/>
<pin name="AD2"/>
<pin name="AD1"/>
<pin name="AD0"/>
<pin name="INT" direction="out"/>
<pin name="BUSY" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="RESET" direction="in"/>
<pin name="READY" direction="in"/>
<pin name="BHE/S7" function="dot"/>
<pin name="S2" function="dot"/>
<pin name="S1" function="dot"/>
<pin name="S0" function="dot"/>
<pin name="RQ/GT0" function="dot"/>
<pin name="QS0" direction="in"/>
<pin name="RQ/GT1" function="dot"/>
<pin name="QS1" direction="in"/>
</symbol>
<symbol name="PWR2GND">
<pin name="VCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="8086MAX">
<pin name="AD14"/>
<pin name="AD13"/>
<pin name="AD12"/>
<pin name="AD11"/>
<pin name="AD10"/>
<pin name="AD9"/>
<pin name="AD8"/>
<pin name="AD7"/>
<pin name="AD6"/>
<pin name="AD5"/>
<pin name="AD4"/>
<pin name="AD3"/>
<pin name="AD2"/>
<pin name="AD1"/>
<pin name="AD0"/>
<pin name="NMI" direction="in"/>
<pin name="INTR" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="RESET" direction="in"/>
<pin name="READY" direction="in"/>
<pin name="TEST" direction="in" function="dot"/>
<pin name="QS1" direction="out"/>
<pin name="QS0" direction="out"/>
<pin name="S0" direction="out" function="dot"/>
<pin name="S1" direction="out" function="dot"/>
<pin name="S2" direction="out" function="dot"/>
<pin name="LOCK" direction="out" function="dot"/>
<pin name="RQ/GT1" function="dot"/>
<pin name="RQ/GT0" function="dot"/>
<pin name="RD" direction="out" function="dot"/>
<pin name="!MX" direction="in"/>
<pin name="!BHE!/S7" direction="out"/>
<pin name="A19/S6" direction="out"/>
<pin name="A18/S5" direction="out"/>
<pin name="A17/S4" direction="out"/>
<pin name="A16/S3" direction="out"/>
<pin name="AD15"/>
</symbol>
<symbol name="8051">
<pin name="XTAL2" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="EA" direction="in"/>
<pin name="P27-A15"/>
<pin name="P26-A14"/>
<pin name="P25-A13"/>
<pin name="P24-A12"/>
<pin name="P23-A11"/>
<pin name="P22-A10"/>
<pin name="P21-A9"/>
<pin name="P20-A8"/>
<pin name="P07-AD7"/>
<pin name="P06-AD6"/>
<pin name="P05-AD5"/>
<pin name="P04-AD4"/>
<pin name="P03-AD3"/>
<pin name="P02-AD2"/>
<pin name="P01-AD1"/>
<pin name="P00-AD0"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out"/>
<pin name="P37-RD"/>
<pin name="P36-WR"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="P11-T2EX"/>
<pin name="RST" direction="in"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P30-RXD"/>
<pin name="P31-TXD"/>
<pin name="P32-INT0"/>
<pin name="P33-INT1"/>
<pin name="P34-T0"/>
<pin name="P35-T1"/>
<pin name="P12"/>
<pin name="P10-T2"/>
</symbol>
<symbol name="75160">
<pin name="PE" direction="in"/>
<pin name="TE" direction="in"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="75161">
<pin name="DC" direction="in"/>
<pin name="TE" direction="in"/>
<pin name="ATN"/>
<pin name="EOI"/>
<pin name="SRQ"/>
<pin name="REN"/>
<pin name="IFC"/>
<pin name="DAV"/>
<pin name="NDAC"/>
<pin name="NRFD"/>
<pin name="ATN2"/>
<pin name="EOI2"/>
<pin name="SRQ2"/>
<pin name="REN2"/>
<pin name="IFC2"/>
<pin name="DAV2"/>
<pin name="NDAC2"/>
<pin name="NRFD2"/>
</symbol>
<symbol name="75162">
<pin name="DC" direction="in"/>
<pin name="TE" direction="in"/>
<pin name="ATN"/>
<pin name="EOI"/>
<pin name="SRQ"/>
<pin name="REN"/>
<pin name="IFC"/>
<pin name="DAV"/>
<pin name="NDAC"/>
<pin name="NRFD"/>
<pin name="ATN2"/>
<pin name="EOI2"/>
<pin name="SRQ2"/>
<pin name="REN2"/>
<pin name="IFC2"/>
<pin name="DAV2"/>
<pin name="NDAC2"/>
<pin name="NRFD2"/>
<pin name="SC" direction="in"/>
<pin name="NC"/>
</symbol>
<symbol name="TMS9914A">
<pin name="DIO8"/>
<pin name="DIO7"/>
<pin name="DIO6"/>
<pin name="DIO5"/>
<pin name="DIO4"/>
<pin name="DIO3"/>
<pin name="DIO2"/>
<pin name="DIO1"/>
<pin name="TE" direction="out"/>
<pin name="/CONT"/>
<pin name="/REN"/>
<pin name="/IFC"/>
<pin name="/NDAC"/>
<pin name="/NRFD"/>
<pin name="/DAV"/>
<pin name="/EOI"/>
<pin name="/ATN"/>
<pin name="/SRQ"/>
<pin name="TR"/>
<pin name="RS0" direction="in"/>
<pin name="RS1" direction="in"/>
<pin name="RS2" direction="in"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="/RESET" direction="in"/>
<pin name="/INT" direction="out"/>
<pin name="/WE" direction="in"/>
<pin name="/ACCRQ" direction="out"/>
<pin name="/CE" direction="in"/>
<pin name="/ACCGR" direction="in"/>
<pin name="DBIN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="4164">
<pin name="DIN" direction="in"/>
<pin name="!WE" direction="in"/>
<pin name="!RAS" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="Q" direction="hiz"/>
<pin name="!CAS" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="80130">
<pin name="BAUD"/>
<pin name="DELAY"/>
<pin name="SYSTICK"/>
<pin name="AD15"/>
<pin name="AD14"/>
<pin name="AD13"/>
<pin name="AD12"/>
<pin name="AD11"/>
<pin name="AD10"/>
<pin name="AD9"/>
<pin name="AD8"/>
<pin name="AD7"/>
<pin name="AD6"/>
<pin name="AD5"/>
<pin name="AD4"/>
<pin name="AD3"/>
<pin name="AD2"/>
<pin name="AD1"/>
<pin name="AD0"/>
<pin name="INT" direction="out"/>
<pin name="ACK" direction="out" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="IR0" direction="in"/>
<pin name="BHE/S7" function="dot"/>
<pin name="S2" function="dot"/>
<pin name="S1" function="dot"/>
<pin name="S0" function="dot"/>
<pin name="MEMCS!" function="dot"/>
<pin name="IOCS" function="dot"/>
<pin name="IR1" direction="in"/>
<pin name="IR2" direction="in"/>
<pin name="IR3" direction="in"/>
<pin name="IR4" direction="in"/>
<pin name="IR5" direction="in"/>
<pin name="IR6" direction="in"/>
<pin name="IR7" direction="in"/>
<pin name="LIR" direction="out" function="dot"/>
</symbol>
<symbol name="74257">
<pin name="!A!/B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="hiz"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="hiz"/>
<pin name="3Y" direction="hiz"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="4Y" direction="hiz"/>
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="PWRN-1">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="20X8">
<pin name="CLK" direction="in" function="clk"/>
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
<pin name="I8" direction="in"/>
<pin name="I9" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="O9" function="dot"/>
<pin name="O8" direction="hiz" function="dot"/>
<pin name="O7" direction="hiz" function="dot"/>
<pin name="O6" direction="hiz" function="dot"/>
<pin name="O5" direction="hiz" function="dot"/>
<pin name="O4" direction="hiz" function="dot"/>
<pin name="O3" direction="hiz" function="dot"/>
<pin name="O2" direction="hiz" function="dot"/>
<pin name="O1" direction="hiz" function="dot"/>
<pin name="O0" function="dot"/>
</symbol>
<symbol name="PWRN-2">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="16R6">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="O0" function="dot"/>
<pin name="O1" direction="out" function="dot"/>
<pin name="O2" direction="out" function="dot"/>
<pin name="O3" direction="out" function="dot"/>
<pin name="O4" direction="out" function="dot"/>
<pin name="O5" direction="out" function="dot"/>
<pin name="O6" direction="out" function="dot"/>
<pin name="O7" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="16R4">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="O0" function="dot"/>
<pin name="O1" function="dot"/>
<pin name="O2" direction="out" function="dot"/>
<pin name="O3" direction="out" function="dot"/>
<pin name="O4" direction="out" function="dot"/>
<pin name="O5" direction="out" function="dot"/>
<pin name="O6" function="dot"/>
<pin name="O7" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="74245">
<pin name="DIR" direction="in"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="74166">
<pin name="SER" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="INH" direction="in" function="clk"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="QH" direction="out"/>
<pin name="H" direction="in"/>
<pin name="SH/!LD" direction="in"/>
</symbol>
<symbol name="7404">
<pin name="I" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="7408">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7410">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I2" direction="in"/>
</symbol>
<symbol name="7430">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
</symbol>
<symbol name="74109">
<pin name="CLR" direction="in" function="dot"/>
<pin name="J" direction="in"/>
<pin name="K" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="74138">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="G2A" direction="in" function="dot"/>
<pin name="G2B" direction="in" function="dot"/>
<pin name="G1" direction="in"/>
<pin name="Y7" direction="out" function="dot"/>
<pin name="Y6" direction="out" function="dot"/>
<pin name="Y5" direction="out" function="dot"/>
<pin name="Y4" direction="out" function="dot"/>
<pin name="Y3" direction="out" function="dot"/>
<pin name="Y2" direction="out" function="dot"/>
<pin name="Y1" direction="out" function="dot"/>
<pin name="Y0" direction="out" function="dot"/>
</symbol>
<symbol name="74156">
<pin name="1C" direction="in"/>
<pin name="1G" direction="in" function="dot"/>
<pin name="B" direction="in"/>
<pin name="1Y3" direction="oc" function="dot"/>
<pin name="1Y2" direction="oc" function="dot"/>
<pin name="1Y1" direction="oc" function="dot"/>
<pin name="1Y0" direction="oc" function="dot"/>
<pin name="2Y0" direction="oc" function="dot"/>
<pin name="2Y1" direction="oc" function="dot"/>
<pin name="2Y2" direction="oc" function="dot"/>
<pin name="2Y3" direction="oc" function="dot"/>
<pin name="A" direction="in"/>
<pin name="2G" direction="in" function="dot"/>
<pin name="2C" direction="in" function="dot"/>
</symbol>
<symbol name="74573">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="8288">
<pin name="!AIOWC" direction="out"/>
<pin name="!AMWC" direction="out"/>
<pin name="!IOWC" direction="out"/>
<pin name="!MWTC" direction="out"/>
<pin name="!MRDC" direction="out"/>
<pin name="!IORC" direction="out"/>
<pin name="!INTA" direction="out"/>
<pin name="DT/!R" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="MCE/!PDEN" direction="out"/>
<pin name="DEN" direction="out"/>
<pin name="!S0" direction="in"/>
<pin name="!S1" direction="in"/>
<pin name="!S2" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="!AEN" direction="in"/>
<pin name="IOB" direction="in"/>
<pin name="CEN" direction="in"/>
</symbol>
<symbol name="8284">
<pin name="!RES" direction="in"/>
<pin name="RESET" direction="out"/>
<pin name="OSC" direction="out" function="clk"/>
<pin name="PCLK" direction="out" function="clk"/>
<pin name="CLK" direction="out" function="clk"/>
<pin name="READY" direction="out"/>
<pin name="X1" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="!AEN1" direction="in"/>
<pin name="!AEN2" direction="in"/>
<pin name="!RDY1" direction="in"/>
<pin name="!RDY2" direction="in"/>
<pin name="!ASYNC" direction="in"/>
<pin name="F/!C" direction="in"/>
<pin name="EFI" direction="in"/>
<pin name="CSYNC" direction="in"/>
</symbol>
<symbol name="7220">
<pin name="!RESET" direction="in"/>
<pin name="!WAIT"/>
<pin name="!DET.ON" direction="out"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="A0" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!DACK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="DRQ" direction="out"/>
<pin name="INT" direction="out"/>
<pin name="!BUS.RD" direction="out"/>
<pin name="CLK" direction="in"/>
<pin name="!PWR.FAIL" direction="in"/>
<pin name="!RESET.OUT" direction="out"/>
<pin name="!ERR.FLG"/>
<pin name="!X+" direction="out"/>
<pin name="!X-" direction="out"/>
<pin name="!Y+" direction="out"/>
<pin name="!Y-" direction="out"/>
<pin name="!TM.A" direction="out"/>
<pin name="!TM.B" direction="out"/>
<pin name="!BOOT.EN" direction="out"/>
<pin name="!SWAP.EN" direction="out"/>
<pin name="C/!D" direction="out"/>
<pin name="!SHIFT.CLK" direction="out"/>
<pin name="!SYNC" direction="out"/>
<pin name="DIO"/>
<pin name="!REP.EN" direction="out"/>
<pin name="!BOOT.SW.EN" direction="out"/>
</symbol>
<symbol name="VDD">
<pin name="VDD" direction="sup"/>
</symbol>
<symbol name="7230">
<pin name="!CS" direction="in"/>
<pin name="!TM.A" direction="in"/>
<pin name="!TM.B" direction="in"/>
<pin name="!REP.EN" direction="in"/>
<pin name="!BOOT.EN" direction="in"/>
<pin name="!GEN.EN.A" direction="in"/>
<pin name="!GEN.EN.B" direction="in"/>
<pin name="!SWAP.EN" direction="in"/>
<pin name="!BOOT.SW.EN" direction="in"/>
<pin name="!PWR.FAIL" direction="out"/>
<pin name="REP.A" direction="out"/>
<pin name="REP.B" direction="out"/>
<pin name="BOOT.REP" direction="out"/>
<pin name="GEN.A" direction="out"/>
<pin name="GEN.B" direction="out"/>
<pin name="SWAP" direction="out"/>
<pin name="BOOT.SW" direction="out"/>
<pin name="REF.RES" direction="in"/>
</symbol>
<symbol name="7242">
<pin name="C/!D" direction="in"/>
<pin name="!SELECT.IN" direction="in"/>
<pin name="!SELECT.OUT" direction="out"/>
<pin name="!ERR.FLG" direction="out"/>
<pin name="DIO"/>
<pin name="!ENABLE.A" direction="out"/>
<pin name="!ENABLE.B" direction="out"/>
<pin name="!DATA.OUT.A" direction="out"/>
<pin name="!DET.A+" direction="in"/>
<pin name="!DET.A-" direction="in"/>
<pin name="!SHIFT.CLK" direction="in"/>
<pin name="!DET.B+" direction="in"/>
<pin name="!DET.B-" direction="in"/>
<pin name="!DATA.OUT.B" direction="out"/>
<pin name="CLK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!RESET" direction="in"/>
</symbol>
<symbol name="7250">
<pin name="!X+.IN" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!X-.IN" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="!Y+.IN" direction="in"/>
<pin name="!Y-.IN" direction="in"/>
<pin name="X+.OUT" direction="out"/>
<pin name="!X+.OUT" direction="out"/>
<pin name="!X-.OUT" direction="out"/>
<pin name="X-.OUT" direction="out"/>
<pin name="Y+.OUT" direction="out"/>
<pin name="!Y+.OUT" direction="out"/>
<pin name="!Y-.OUT" direction="out"/>
<pin name="Y-.OUT" direction="out"/>
</symbol>
<symbol name="7254">
<pin name="G4" direction="in"/>
<pin name="G3" direction="in"/>
<pin name="G1" direction="in"/>
<pin name="G2" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="S3" direction="pwr"/>
<pin name="S1" direction="pwr"/>
<pin name="S2" direction="pwr"/>
<pin name="S4" direction="pwr"/>
<pin name="NC1" direction="nc"/>
<pin name="D2" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
</symbol>
<symbol name="LABELED-PMOS">
<description>&lt;h3&gt;P-channel MOSFET&lt;/h3&gt;
Switches electrical signals</description>
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
<symbol name="LABELED-NMOS">
<description>&lt;h3&gt; N-channel MOSFET transistor&lt;/h3&gt;
Switches electronic signals</description>
<pin name="G"/>
<pin name="S"/>
<pin name="D"/>
</symbol>
<symbol name="7110">
<pin name="PULSE.COM" direction="pwr"/>
<pin name="REPLICATE.B" direction="in"/>
<pin name="REPLICATE.A" direction="in"/>
<pin name="BOOT.REP" direction="in"/>
<pin name="BOOT.SWAP" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="GENERATE.A" direction="in"/>
<pin name="GENERATE.B" direction="in"/>
<pin name="X-.COIL.IN" direction="in"/>
<pin name="X+.COIL.IN" direction="in"/>
<pin name="DET.SUPPLY" direction="pwr"/>
<pin name="DET.OUT.A+" direction="out"/>
<pin name="DET.OUT.A-" direction="out"/>
<pin name="DET.OUT.B+" direction="out"/>
<pin name="DET.OUT.B-" direction="out"/>
<pin name="DET.COM" direction="pwr"/>
<pin name="SWAP.B" direction="in"/>
<pin name="SWAP.A" direction="in"/>
<pin name="Y+.COIL.IN" direction="in"/>
<pin name="Y-.COIL.IN" direction="in"/>
</symbol>
<symbol name="OR">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="PWRN-3">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="SN75160BDW">
<pin name="VCC" direction="pwr"/>
<pin name="TE" direction="in"/>
<pin name="PE" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="B7" direction="out"/>
</symbol>
<symbol name="SN75160BDWR">
<pin name="VCC" direction="pwr"/>
<pin name="TE" direction="in"/>
<pin name="PE" direction="in"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="GND" direction="pas"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
</symbol>
<symbol name="SN75160BN">
<pin name="VCC" direction="pwr"/>
<pin name="TE" direction="in"/>
<pin name="PE" direction="in"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="GND" direction="pas"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
</symbol>
<symbol name="SN75161BDW">
<pin name="VCC" direction="pwr"/>
<pin name="DC" direction="in"/>
<pin name="ATN_2" direction="in"/>
<pin name="SRQ_2" direction="in"/>
<pin name="DAV_2" direction="in"/>
<pin name="NDAC_2" direction="in"/>
<pin name="IFC_2" direction="in"/>
<pin name="NRFD_2" direction="in"/>
<pin name="TE" direction="in"/>
<pin name="EOI_2" direction="in"/>
<pin name="REN_2" direction="in"/>
<pin name="SRQ" direction="in"/>
<pin name="REN" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="NDAC" direction="out"/>
<pin name="DAV" direction="out"/>
<pin name="EOI" direction="out"/>
<pin name="NRFD" direction="out"/>
<pin name="ATN" direction="out"/>
<pin name="IFC" direction="out"/>
</symbol>
<symbol name="SN75161BN">
<pin name="VCC" direction="pwr"/>
<pin name="TE" direction="in"/>
<pin name="DC" direction="in"/>
<pin name="REN_2"/>
<pin name="SRQ_2"/>
<pin name="IFC_2"/>
<pin name="NDAC_2"/>
<pin name="NRFD_2"/>
<pin name="DAV_2"/>
<pin name="EOI_2"/>
<pin name="ATN_2"/>
<pin name="GND" direction="pas"/>
<pin name="REN"/>
<pin name="SRQ"/>
<pin name="IFC"/>
<pin name="NDAC"/>
<pin name="NRFD"/>
<pin name="DAV"/>
<pin name="EOI"/>
<pin name="ATN"/>
</symbol>
<symbol name="SN75162BDW">
<pin name="VCC" direction="pwr"/>
<pin name="REN_2"/>
<pin name="TE"/>
<pin name="IFC_2"/>
<pin name="SC"/>
<pin name="ATN_2"/>
<pin name="SRQ_2"/>
<pin name="NRFD_2"/>
<pin name="EOI_2"/>
<pin name="DC" direction="pas"/>
<pin name="NC_2" direction="nc"/>
<pin name="NC_3" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="GND" direction="pas"/>
<pin name="SRQ"/>
<pin name="NDAC_2"/>
<pin name="NRFD"/>
<pin name="NDAC"/>
<pin name="ATN"/>
<pin name="IFC"/>
<pin name="REN"/>
<pin name="DAV_2"/>
<pin name="EOI"/>
<pin name="DAV"/>
</symbol>
<symbol name="24G">
<pin name="G" direction="pas"/>
<pin name="G1" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
</symbol>
<symbol name="GPIB-PINHD-2X12">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
</symbol>
<symbol name="RASPBERRY-PI+">
<pin name="1-3V3"/>
<pin name="2-5V"/>
<pin name="3-SDA1/GPIO2"/>
<pin name="4-5V"/>
<pin name="5-SCL1/GPIO3"/>
<pin name="6-GND"/>
<pin name="7-GPIO4"/>
<pin name="8-TX"/>
<pin name="9-GND"/>
<pin name="10-RX"/>
<pin name="11-GPIO17"/>
<pin name="12-GPIO18"/>
<pin name="13-GPIO27"/>
<pin name="14-GND"/>
<pin name="15-GPIO22"/>
<pin name="16-GPIO23"/>
<pin name="17-3V3"/>
<pin name="18-GPIO24"/>
<pin name="19-SPI-MOSI/GPIO10"/>
<pin name="20-GND"/>
<pin name="21-SPI-MISO/GPIO9"/>
<pin name="22-GPIO25"/>
<pin name="23-SPI-SCLK/GPIO11"/>
<pin name="24-GPIO8"/>
<pin name="25-GND"/>
<pin name="26-GPIO7"/>
<pin name="27-ID_SD"/>
<pin name="29-GPIO5"/>
<pin name="31-GPIO6"/>
<pin name="33-GPIO13"/>
<pin name="35-GPIO19"/>
<pin name="37-GPIO26"/>
<pin name="39-GND"/>
<pin name="28-ID_SC"/>
<pin name="30-GND"/>
<pin name="32-GPIO12"/>
<pin name="34-GND"/>
<pin name="36-GPIO16"/>
<pin name="38-GPIO20"/>
<pin name="40-GPIO21"/>
</symbol>
<symbol name="2764">
<pin name="VPP" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="O0" direction="hiz"/>
<pin name="O1" direction="hiz"/>
<pin name="O2" direction="hiz"/>
<pin name="O3" direction="hiz"/>
<pin name="O4" direction="hiz"/>
<pin name="O5" direction="hiz"/>
<pin name="O6" direction="hiz"/>
<pin name="O7" direction="hiz"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="!PGM" direction="in"/>
</symbol>
<symbol name="PWRN-4">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="RN4">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="MM58174">
<pin name="!CS" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="DB3"/>
<pin name="DB2"/>
<pin name="DB1"/>
<pin name="DB0"/>
<pin name="VSS" direction="pwr"/>
<pin name="AD3" direction="in"/>
<pin name="AD2" direction="in"/>
<pin name="AD1" direction="in"/>
<pin name="AD0" direction="in"/>
<pin name="!INT" direction="out"/>
<pin name="XO" direction="out"/>
<pin name="XI" direction="in"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="X2210D">
<pin name="NC" direction="nc"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="!STORE" direction="in"/>
<pin name="!RECALL" direction="in"/>
<pin name="!WE" direction="in"/>
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="A5" direction="in"/>
<pin name="NC1" direction="nc"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="+UB">
<pin name="+UB" direction="pwr"/>
</symbol>
<symbol name="-UB">
<pin name="-UB" direction="pwr"/>
</symbol>
<symbol name="161">
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="CLK" direction="in"/>
<pin name="ENP" direction="in"/>
<pin name="ENT" direction="in"/>
<pin name="!LOAD" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="RCO" direction="out"/>
</symbol>
<symbol name="163">
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="CLK" direction="in"/>
<pin name="ENP" direction="in"/>
<pin name="ENT" direction="in"/>
<pin name="!LOAD" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="RCO" direction="out"/>
</symbol>
<symbol name="PAD-N">
</symbol>
<symbol name="8274">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLK" function="clk"/>
<pin name="!RESET" function="dot"/>
<pin name="RDYB/TXDRQA" direction="out"/>
<pin name="RDYA/RXDRQA" direction="out"/>
<pin name="TXDRQB/!IPO" direction="out"/>
<pin name="TRXDRQB/!IPI"/>
<pin name="!INT" direction="out" function="dot"/>
<pin name="!INTA" direction="in" function="dot"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!CS" direction="in" function="dot"/>
<pin name="!RD" direction="in" function="dot"/>
<pin name="!WR" direction="in" function="dot"/>
<pin name="TXDA" direction="out"/>
<pin name="!TXCA" direction="in" function="dot"/>
<pin name="!CDA" direction="in" function="dot"/>
<pin name="!CTSA" direction="in" function="dot"/>
<pin name="!RTSA" direction="out" function="dot"/>
<pin name="!SYNDETA" direction="out" function="dot"/>
<pin name="!DRTA" direction="out" function="dot"/>
<pin name="RXDA" direction="in"/>
<pin name="!RXCA" direction="in" function="dot"/>
<pin name="TXDB" direction="out"/>
<pin name="!TXCB" direction="in" function="dot"/>
<pin name="!CDB" direction="in" function="dot"/>
<pin name="!CTSB" direction="in" function="dot"/>
<pin name="!SYNDETB/RTSB" direction="out" function="dot"/>
<pin name="!DRTB" direction="out" function="dot"/>
<pin name="RXDB" direction="in"/>
<pin name="!RXCB" direction="in" function="dot"/>
</symbol>
<symbol name="PINH2X5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X12">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X17">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
<pin name="21" direction="pas" function="dot"/>
<pin name="22" direction="pas" function="dot"/>
<pin name="23" direction="pas" function="dot"/>
<pin name="24" direction="pas" function="dot"/>
<pin name="25" direction="pas" function="dot"/>
<pin name="26" direction="pas" function="dot"/>
<pin name="27" direction="pas" function="dot"/>
<pin name="28" direction="pas" function="dot"/>
<pin name="29" direction="pas" function="dot"/>
<pin name="30" direction="pas" function="dot"/>
<pin name="31" direction="pas" function="dot"/>
<pin name="32" direction="pas" function="dot"/>
<pin name="33" direction="pas" function="dot"/>
<pin name="34" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X10">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="17" direction="pas" function="dot"/>
<pin name="18" direction="pas" function="dot"/>
<pin name="19" direction="pas" function="dot"/>
<pin name="20" direction="pas" function="dot"/>
</symbol>
<symbol name="4194">
<pin name="VIN+" direction="pwr"/>
<pin name="VIN-" direction="pwr"/>
<pin name="RSET" direction="pas"/>
<pin name="COMP-" direction="pas"/>
<pin name="COMP+" direction="pas"/>
<pin name="GND"/>
<pin name="RO" direction="pas"/>
<pin name="VO-"/>
<pin name="BAL" direction="pas"/>
<pin name="VO+"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="MC3488">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="WS" direction="pas"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="!OUTA" direction="out" function="dot"/>
<pin name="!OUTB" direction="out" function="dot"/>
</symbol>
<symbol name="7405">
<pin name="I" direction="in"/>
<pin name="O" direction="oc" function="dot"/>
</symbol>
<symbol name="7414">
<pin name="I" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="74259">
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="D" direction="in"/>
<pin name="G" direction="in" function="dot"/>
<pin name="CLR" direction="in" function="dot"/>
</symbol>
<symbol name="16L8">
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
<pin name="I8" direction="in"/>
<pin name="I9" direction="in"/>
<pin name="O0" direction="out" function="dot"/>
<pin name="O1" function="dot"/>
<pin name="O2" function="dot"/>
<pin name="O3" function="dot"/>
<pin name="O4" function="dot"/>
<pin name="O5" function="dot"/>
<pin name="O6" function="dot"/>
<pin name="O7" direction="out" function="dot"/>
<pin name="I0" direction="in"/>
</symbol>
<symbol name="QG3">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="TS" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="8087" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MICROCOMPUTER/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8087"/>
<gate name="P" symbol="PWR2GND"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="A16/S3" pad="38"/>
<connect gate="G$1" pin="A17/S4" pad="37"/>
<connect gate="G$1" pin="A18/S5" pad="36"/>
<connect gate="G$1" pin="A19/S6" pad="35"/>
<connect gate="G$1" pin="AD0" pad="16"/>
<connect gate="G$1" pin="AD1" pad="15"/>
<connect gate="G$1" pin="AD10" pad="6"/>
<connect gate="G$1" pin="AD11" pad="5"/>
<connect gate="G$1" pin="AD12" pad="4"/>
<connect gate="G$1" pin="AD13" pad="3"/>
<connect gate="G$1" pin="AD14" pad="2"/>
<connect gate="G$1" pin="AD15" pad="39"/>
<connect gate="G$1" pin="AD2" pad="14"/>
<connect gate="G$1" pin="AD3" pad="13"/>
<connect gate="G$1" pin="AD4" pad="12"/>
<connect gate="G$1" pin="AD5" pad="11"/>
<connect gate="G$1" pin="AD6" pad="10"/>
<connect gate="G$1" pin="AD7" pad="9"/>
<connect gate="G$1" pin="AD8" pad="8"/>
<connect gate="G$1" pin="AD9" pad="7"/>
<connect gate="G$1" pin="BHE/S7" pad="34"/>
<connect gate="G$1" pin="BUSY" pad="23"/>
<connect gate="G$1" pin="CLK" pad="19"/>
<connect gate="G$1" pin="INT" pad="32"/>
<connect gate="G$1" pin="QS0" pad="25"/>
<connect gate="G$1" pin="QS1" pad="24"/>
<connect gate="G$1" pin="READY" pad="22"/>
<connect gate="G$1" pin="RESET" pad="21"/>
<connect gate="G$1" pin="RQ/GT0" pad="31"/>
<connect gate="G$1" pin="RQ/GT1" pad="33"/>
<connect gate="G$1" pin="S0" pad="26"/>
<connect gate="G$1" pin="S1" pad="27"/>
<connect gate="G$1" pin="S2" pad="28"/>
<connect gate="P" pin="GND@1" pad="1"/>
<connect gate="P" pin="GND@2" pad="20"/>
<connect gate="P" pin="VCC" pad="40"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8086MAX" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MICROCOMPUTER/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="8086MAX"/>
<gate name="P" symbol="PWR2GND"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="A" pin="!BHE!/S7" pad="34"/>
<connect gate="A" pin="!MX" pad="33"/>
<connect gate="A" pin="A16/S3" pad="38"/>
<connect gate="A" pin="A17/S4" pad="37"/>
<connect gate="A" pin="A18/S5" pad="36"/>
<connect gate="A" pin="A19/S6" pad="35"/>
<connect gate="A" pin="AD0" pad="16"/>
<connect gate="A" pin="AD1" pad="15"/>
<connect gate="A" pin="AD10" pad="6"/>
<connect gate="A" pin="AD11" pad="5"/>
<connect gate="A" pin="AD12" pad="4"/>
<connect gate="A" pin="AD13" pad="3"/>
<connect gate="A" pin="AD14" pad="2"/>
<connect gate="A" pin="AD15" pad="39"/>
<connect gate="A" pin="AD2" pad="14"/>
<connect gate="A" pin="AD3" pad="13"/>
<connect gate="A" pin="AD4" pad="12"/>
<connect gate="A" pin="AD5" pad="11"/>
<connect gate="A" pin="AD6" pad="10"/>
<connect gate="A" pin="AD7" pad="9"/>
<connect gate="A" pin="AD8" pad="8"/>
<connect gate="A" pin="AD9" pad="7"/>
<connect gate="A" pin="CLK" pad="19"/>
<connect gate="A" pin="INTR" pad="18"/>
<connect gate="A" pin="LOCK" pad="29"/>
<connect gate="A" pin="NMI" pad="17"/>
<connect gate="A" pin="QS0" pad="25"/>
<connect gate="A" pin="QS1" pad="24"/>
<connect gate="A" pin="RD" pad="32"/>
<connect gate="A" pin="READY" pad="22"/>
<connect gate="A" pin="RESET" pad="21"/>
<connect gate="A" pin="RQ/GT0" pad="31"/>
<connect gate="A" pin="RQ/GT1" pad="30"/>
<connect gate="A" pin="S0" pad="26"/>
<connect gate="A" pin="S1" pad="27"/>
<connect gate="A" pin="S2" pad="28"/>
<connect gate="A" pin="TEST" pad="23"/>
<connect gate="P" pin="GND@1" pad="1"/>
<connect gate="P" pin="GND@2" pad="20"/>
<connect gate="P" pin="VCC" pad="40"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8051" prefix="IC">
<description>&lt;b&gt;(CHMOS) SINGLE-CHIP 8-BIT MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
80C31BH / 80C51 BH / 87C51 MCS 51&lt;br&gt;
Source: http://apps.intel.com .. 27041907.pdf</description>
<gates>
<gate name="G$1" symbol="8051"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="EA" pad="31"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="P00-AD0" pad="39"/>
<connect gate="G$1" pin="P01-AD1" pad="38"/>
<connect gate="G$1" pin="P02-AD2" pad="37"/>
<connect gate="G$1" pin="P03-AD3" pad="36"/>
<connect gate="G$1" pin="P04-AD4" pad="35"/>
<connect gate="G$1" pin="P05-AD5" pad="34"/>
<connect gate="G$1" pin="P06-AD6" pad="33"/>
<connect gate="G$1" pin="P07-AD7" pad="32"/>
<connect gate="G$1" pin="P10-T2" pad="1"/>
<connect gate="G$1" pin="P11-T2EX" pad="2"/>
<connect gate="G$1" pin="P12" pad="3"/>
<connect gate="G$1" pin="P13" pad="4"/>
<connect gate="G$1" pin="P14" pad="5"/>
<connect gate="G$1" pin="P15" pad="6"/>
<connect gate="G$1" pin="P16" pad="7"/>
<connect gate="G$1" pin="P17" pad="8"/>
<connect gate="G$1" pin="P20-A8" pad="21"/>
<connect gate="G$1" pin="P21-A9" pad="22"/>
<connect gate="G$1" pin="P22-A10" pad="23"/>
<connect gate="G$1" pin="P23-A11" pad="24"/>
<connect gate="G$1" pin="P24-A12" pad="25"/>
<connect gate="G$1" pin="P25-A13" pad="26"/>
<connect gate="G$1" pin="P26-A14" pad="27"/>
<connect gate="G$1" pin="P27-A15" pad="28"/>
<connect gate="G$1" pin="P30-RXD" pad="10"/>
<connect gate="G$1" pin="P31-TXD" pad="11"/>
<connect gate="G$1" pin="P32-INT0" pad="12"/>
<connect gate="G$1" pin="P33-INT1" pad="13"/>
<connect gate="G$1" pin="P34-T0" pad="14"/>
<connect gate="G$1" pin="P35-T1" pad="15"/>
<connect gate="G$1" pin="P36-WR" pad="16"/>
<connect gate="G$1" pin="P37-RD" pad="17"/>
<connect gate="G$1" pin="PSEN" pad="29"/>
<connect gate="G$1" pin="RST" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="N" package="PLCC44">
<connects>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="EA" pad="35"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="P00-AD0" pad="43"/>
<connect gate="G$1" pin="P01-AD1" pad="42"/>
<connect gate="G$1" pin="P02-AD2" pad="41"/>
<connect gate="G$1" pin="P03-AD3" pad="40"/>
<connect gate="G$1" pin="P04-AD4" pad="39"/>
<connect gate="G$1" pin="P05-AD5" pad="38"/>
<connect gate="G$1" pin="P06-AD6" pad="37"/>
<connect gate="G$1" pin="P07-AD7" pad="36"/>
<connect gate="G$1" pin="P10-T2" pad="2"/>
<connect gate="G$1" pin="P11-T2EX" pad="3"/>
<connect gate="G$1" pin="P12" pad="4"/>
<connect gate="G$1" pin="P13" pad="5"/>
<connect gate="G$1" pin="P14" pad="6"/>
<connect gate="G$1" pin="P15" pad="7"/>
<connect gate="G$1" pin="P16" pad="8"/>
<connect gate="G$1" pin="P17" pad="9"/>
<connect gate="G$1" pin="P20-A8" pad="24"/>
<connect gate="G$1" pin="P21-A9" pad="25"/>
<connect gate="G$1" pin="P22-A10" pad="26"/>
<connect gate="G$1" pin="P23-A11" pad="27"/>
<connect gate="G$1" pin="P24-A12" pad="28"/>
<connect gate="G$1" pin="P25-A13" pad="29"/>
<connect gate="G$1" pin="P26-A14" pad="30"/>
<connect gate="G$1" pin="P27-A15" pad="31"/>
<connect gate="G$1" pin="P30-RXD" pad="11"/>
<connect gate="G$1" pin="P31-TXD" pad="13"/>
<connect gate="G$1" pin="P32-INT0" pad="14"/>
<connect gate="G$1" pin="P33-INT1" pad="15"/>
<connect gate="G$1" pin="P34-T0" pad="16"/>
<connect gate="G$1" pin="P35-T1" pad="17"/>
<connect gate="G$1" pin="P36-WR" pad="18"/>
<connect gate="G$1" pin="P37-RD" pad="19"/>
<connect gate="G$1" pin="PSEN" pad="32"/>
<connect gate="G$1" pin="RST" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="N-SOCK" package="S44">
<connects>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="EA" pad="35"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="P00-AD0" pad="43"/>
<connect gate="G$1" pin="P01-AD1" pad="42"/>
<connect gate="G$1" pin="P02-AD2" pad="41"/>
<connect gate="G$1" pin="P03-AD3" pad="40"/>
<connect gate="G$1" pin="P04-AD4" pad="39"/>
<connect gate="G$1" pin="P05-AD5" pad="38"/>
<connect gate="G$1" pin="P06-AD6" pad="37"/>
<connect gate="G$1" pin="P07-AD7" pad="36"/>
<connect gate="G$1" pin="P10-T2" pad="2"/>
<connect gate="G$1" pin="P11-T2EX" pad="3"/>
<connect gate="G$1" pin="P12" pad="4"/>
<connect gate="G$1" pin="P13" pad="5"/>
<connect gate="G$1" pin="P14" pad="6"/>
<connect gate="G$1" pin="P15" pad="7"/>
<connect gate="G$1" pin="P16" pad="8"/>
<connect gate="G$1" pin="P17" pad="9"/>
<connect gate="G$1" pin="P20-A8" pad="24"/>
<connect gate="G$1" pin="P21-A9" pad="25"/>
<connect gate="G$1" pin="P22-A10" pad="26"/>
<connect gate="G$1" pin="P23-A11" pad="27"/>
<connect gate="G$1" pin="P24-A12" pad="28"/>
<connect gate="G$1" pin="P25-A13" pad="29"/>
<connect gate="G$1" pin="P26-A14" pad="30"/>
<connect gate="G$1" pin="P27-A15" pad="31"/>
<connect gate="G$1" pin="P30-RXD" pad="11"/>
<connect gate="G$1" pin="P31-TXD" pad="13"/>
<connect gate="G$1" pin="P32-INT0" pad="14"/>
<connect gate="G$1" pin="P33-INT1" pad="15"/>
<connect gate="G$1" pin="P34-T0" pad="16"/>
<connect gate="G$1" pin="P35-T1" pad="17"/>
<connect gate="G$1" pin="P36-WR" pad="18"/>
<connect gate="G$1" pin="P37-RD" pad="19"/>
<connect gate="G$1" pin="PSEN" pad="32"/>
<connect gate="G$1" pin="RST" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="75160" prefix="IC" uservalue="yes">
<description>&lt;b&gt;75xxx DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="75160"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="D1" pad="19"/>
<connect gate="G$1" pin="D2" pad="18"/>
<connect gate="G$1" pin="D3" pad="17"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="15"/>
<connect gate="G$1" pin="D6" pad="14"/>
<connect gate="G$1" pin="D7" pad="13"/>
<connect gate="G$1" pin="D8" pad="12"/>
<connect gate="G$1" pin="PE" pad="11"/>
<connect gate="G$1" pin="TE" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO" package="SO20L">
<connects>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="D1" pad="19"/>
<connect gate="G$1" pin="D2" pad="18"/>
<connect gate="G$1" pin="D3" pad="17"/>
<connect gate="G$1" pin="D4" pad="16"/>
<connect gate="G$1" pin="D5" pad="15"/>
<connect gate="G$1" pin="D6" pad="14"/>
<connect gate="G$1" pin="D7" pad="13"/>
<connect gate="G$1" pin="D8" pad="12"/>
<connect gate="G$1" pin="PE" pad="11"/>
<connect gate="G$1" pin="TE" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="75161" prefix="IC">
<description>&lt;b&gt;75xxx DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="75161"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="ATN" pad="13"/>
<connect gate="G$1" pin="ATN2" pad="8"/>
<connect gate="G$1" pin="DAV" pad="15"/>
<connect gate="G$1" pin="DAV2" pad="6"/>
<connect gate="G$1" pin="DC" pad="11"/>
<connect gate="G$1" pin="EOI" pad="14"/>
<connect gate="G$1" pin="EOI2" pad="7"/>
<connect gate="G$1" pin="IFC" pad="18"/>
<connect gate="G$1" pin="IFC2" pad="3"/>
<connect gate="G$1" pin="NDAC" pad="17"/>
<connect gate="G$1" pin="NDAC2" pad="4"/>
<connect gate="G$1" pin="NRFD" pad="16"/>
<connect gate="G$1" pin="NRFD2" pad="5"/>
<connect gate="G$1" pin="REN" pad="19"/>
<connect gate="G$1" pin="REN2" pad="2"/>
<connect gate="G$1" pin="SRQ" pad="12"/>
<connect gate="G$1" pin="SRQ2" pad="9"/>
<connect gate="G$1" pin="TE" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO" package="SO20L">
<connects>
<connect gate="G$1" pin="ATN" pad="13"/>
<connect gate="G$1" pin="ATN2" pad="8"/>
<connect gate="G$1" pin="DAV" pad="15"/>
<connect gate="G$1" pin="DAV2" pad="6"/>
<connect gate="G$1" pin="DC" pad="11"/>
<connect gate="G$1" pin="EOI" pad="14"/>
<connect gate="G$1" pin="EOI2" pad="7"/>
<connect gate="G$1" pin="IFC" pad="18"/>
<connect gate="G$1" pin="IFC2" pad="3"/>
<connect gate="G$1" pin="NDAC" pad="17"/>
<connect gate="G$1" pin="NDAC2" pad="4"/>
<connect gate="G$1" pin="NRFD" pad="16"/>
<connect gate="G$1" pin="NRFD2" pad="5"/>
<connect gate="G$1" pin="REN" pad="19"/>
<connect gate="G$1" pin="REN2" pad="2"/>
<connect gate="G$1" pin="SRQ" pad="12"/>
<connect gate="G$1" pin="SRQ2" pad="9"/>
<connect gate="G$1" pin="TE" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="75162" prefix="IC">
<description>&lt;b&gt;75xxx DEVICE&lt;/b&gt;</description>
<gates>
<gate name="IC" symbol="75162"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="P" package="DIL22-3">
<connects>
<connect gate="IC" pin="ATN" pad="14"/>
<connect gate="IC" pin="ATN2" pad="9"/>
<connect gate="IC" pin="DAV" pad="16"/>
<connect gate="IC" pin="DAV2" pad="7"/>
<connect gate="IC" pin="DC" pad="12"/>
<connect gate="IC" pin="EOI" pad="15"/>
<connect gate="IC" pin="EOI2" pad="8"/>
<connect gate="IC" pin="IFC" pad="19"/>
<connect gate="IC" pin="IFC2" pad="4"/>
<connect gate="IC" pin="NC" pad="21"/>
<connect gate="IC" pin="NDAC" pad="18"/>
<connect gate="IC" pin="NDAC2" pad="5"/>
<connect gate="IC" pin="NRFD" pad="17"/>
<connect gate="IC" pin="NRFD2" pad="6"/>
<connect gate="IC" pin="REN" pad="20"/>
<connect gate="IC" pin="REN2" pad="3"/>
<connect gate="IC" pin="SC" pad="1"/>
<connect gate="IC" pin="SRQ" pad="13"/>
<connect gate="IC" pin="SRQ2" pad="10"/>
<connect gate="IC" pin="TE" pad="2"/>
<connect gate="P" pin="GND" pad="11"/>
<connect gate="P" pin="VCC" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="DIL24-3">
<connects>
<connect gate="IC" pin="ATN" pad="16"/>
<connect gate="IC" pin="ATN2" pad="9"/>
<connect gate="IC" pin="DAV" pad="18"/>
<connect gate="IC" pin="DAV2" pad="7"/>
<connect gate="IC" pin="DC" pad="13"/>
<connect gate="IC" pin="EOI" pad="17"/>
<connect gate="IC" pin="EOI2" pad="8"/>
<connect gate="IC" pin="IFC" pad="21"/>
<connect gate="IC" pin="IFC2" pad="4"/>
<connect gate="IC" pin="NC" pad="11 14 23"/>
<connect gate="IC" pin="NDAC" pad="20"/>
<connect gate="IC" pin="NDAC2" pad="5"/>
<connect gate="IC" pin="NRFD" pad="19"/>
<connect gate="IC" pin="NRFD2" pad="6"/>
<connect gate="IC" pin="REN" pad="22"/>
<connect gate="IC" pin="REN2" pad="3"/>
<connect gate="IC" pin="SC" pad="1"/>
<connect gate="IC" pin="SRQ" pad="15"/>
<connect gate="IC" pin="SRQ2" pad="10"/>
<connect gate="IC" pin="TE" pad="2"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="P1"/>
</technologies>
</device>
<device name="SO24" package="SOIC127P1030X265-24N">
<connects>
<connect gate="IC" pin="ATN" pad="16"/>
<connect gate="IC" pin="ATN2" pad="9"/>
<connect gate="IC" pin="DAV" pad="18"/>
<connect gate="IC" pin="DAV2" pad="7"/>
<connect gate="IC" pin="DC" pad="13"/>
<connect gate="IC" pin="EOI" pad="17"/>
<connect gate="IC" pin="EOI2" pad="8"/>
<connect gate="IC" pin="IFC" pad="21"/>
<connect gate="IC" pin="IFC2" pad="4"/>
<connect gate="IC" pin="NC" pad="11 14 23"/>
<connect gate="IC" pin="NDAC" pad="20"/>
<connect gate="IC" pin="NDAC2" pad="5"/>
<connect gate="IC" pin="NRFD" pad="19"/>
<connect gate="IC" pin="NRFD2" pad="6"/>
<connect gate="IC" pin="REN" pad="22"/>
<connect gate="IC" pin="REN2" pad="3"/>
<connect gate="IC" pin="SC" pad="1"/>
<connect gate="IC" pin="SRQ" pad="15"/>
<connect gate="IC" pin="SRQ2" pad="10"/>
<connect gate="IC" pin="TE" pad="2"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMS9914A" uservalue="yes">
<gates>
<gate name="IC$1" symbol="TMS9914A"/>
</gates>
<devices>
<device name="NL" package="DIL40">
<connects>
<connect gate="IC$1" pin="/ACCGR" pad="2"/>
<connect gate="IC$1" pin="/ACCRQ" pad="1"/>
<connect gate="IC$1" pin="/ATN" pad="28"/>
<connect gate="IC$1" pin="/CE" pad="3"/>
<connect gate="IC$1" pin="/CONT" pad="30"/>
<connect gate="IC$1" pin="/DAV" pad="26"/>
<connect gate="IC$1" pin="/EOI" pad="27"/>
<connect gate="IC$1" pin="/IFC" pad="23"/>
<connect gate="IC$1" pin="/INT" pad="9"/>
<connect gate="IC$1" pin="/NDAC" pad="24"/>
<connect gate="IC$1" pin="/NRFD" pad="25"/>
<connect gate="IC$1" pin="/REN" pad="22"/>
<connect gate="IC$1" pin="/RESET" pad="19"/>
<connect gate="IC$1" pin="/SRQ" pad="29"/>
<connect gate="IC$1" pin="/WE" pad="4"/>
<connect gate="IC$1" pin="CLK" pad="18"/>
<connect gate="IC$1" pin="D0" pad="17"/>
<connect gate="IC$1" pin="D1" pad="16"/>
<connect gate="IC$1" pin="D2" pad="15"/>
<connect gate="IC$1" pin="D3" pad="14"/>
<connect gate="IC$1" pin="D4" pad="13"/>
<connect gate="IC$1" pin="D5" pad="12"/>
<connect gate="IC$1" pin="D6" pad="11"/>
<connect gate="IC$1" pin="D7" pad="10"/>
<connect gate="IC$1" pin="DBIN" pad="5"/>
<connect gate="IC$1" pin="DIO1" pad="38"/>
<connect gate="IC$1" pin="DIO2" pad="37"/>
<connect gate="IC$1" pin="DIO3" pad="36"/>
<connect gate="IC$1" pin="DIO4" pad="35"/>
<connect gate="IC$1" pin="DIO5" pad="34"/>
<connect gate="IC$1" pin="DIO6" pad="33"/>
<connect gate="IC$1" pin="DIO7" pad="32"/>
<connect gate="IC$1" pin="DIO8" pad="31"/>
<connect gate="IC$1" pin="GND" pad="20"/>
<connect gate="IC$1" pin="RS0" pad="6"/>
<connect gate="IC$1" pin="RS1" pad="7"/>
<connect gate="IC$1" pin="RS2" pad="8"/>
<connect gate="IC$1" pin="TE" pad="21"/>
<connect gate="IC$1" pin="TR" pad="39"/>
<connect gate="IC$1" pin="VCC" pad="40"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4164" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G1" symbol="4164"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G1" pin="!CAS" pad="15"/>
<connect gate="G1" pin="!RAS" pad="4"/>
<connect gate="G1" pin="!WE" pad="3"/>
<connect gate="G1" pin="A0" pad="5"/>
<connect gate="G1" pin="A1" pad="7"/>
<connect gate="G1" pin="A2" pad="6"/>
<connect gate="G1" pin="A3" pad="12"/>
<connect gate="G1" pin="A4" pad="11"/>
<connect gate="G1" pin="A5" pad="10"/>
<connect gate="G1" pin="A6" pad="13"/>
<connect gate="G1" pin="A7" pad="9"/>
<connect gate="G1" pin="DIN" pad="2"/>
<connect gate="G1" pin="Q" pad="14"/>
<connect gate="G1" pin="VDD" pad="16"/>
<connect gate="G1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80130" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MICROCOMPUTER/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G1" symbol="80130"/>
<gate name="G2" symbol="PWR2GND"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G1" pin="ACK" pad="25"/>
<connect gate="G1" pin="AD0" pad="16"/>
<connect gate="G1" pin="AD1" pad="15"/>
<connect gate="G1" pin="AD10" pad="6"/>
<connect gate="G1" pin="AD11" pad="5"/>
<connect gate="G1" pin="AD12" pad="4"/>
<connect gate="G1" pin="AD13" pad="3"/>
<connect gate="G1" pin="AD14" pad="2"/>
<connect gate="G1" pin="AD15" pad="39"/>
<connect gate="G1" pin="AD2" pad="14"/>
<connect gate="G1" pin="AD3" pad="13"/>
<connect gate="G1" pin="AD4" pad="12"/>
<connect gate="G1" pin="AD5" pad="11"/>
<connect gate="G1" pin="AD6" pad="10"/>
<connect gate="G1" pin="AD7" pad="9"/>
<connect gate="G1" pin="AD8" pad="8"/>
<connect gate="G1" pin="AD9" pad="7"/>
<connect gate="G1" pin="BAUD" pad="21"/>
<connect gate="G1" pin="BHE/S7" pad="38"/>
<connect gate="G1" pin="CLK" pad="19"/>
<connect gate="G1" pin="DELAY" pad="22"/>
<connect gate="G1" pin="INT" pad="29"/>
<connect gate="G1" pin="IOCS" pad="18"/>
<connect gate="G1" pin="IR0" pad="30"/>
<connect gate="G1" pin="IR1" pad="31"/>
<connect gate="G1" pin="IR2" pad="32"/>
<connect gate="G1" pin="IR3" pad="33"/>
<connect gate="G1" pin="IR4" pad="34"/>
<connect gate="G1" pin="IR5" pad="35"/>
<connect gate="G1" pin="IR6" pad="36"/>
<connect gate="G1" pin="IR7" pad="37"/>
<connect gate="G1" pin="LIR" pad="24"/>
<connect gate="G1" pin="MEMCS!" pad="17"/>
<connect gate="G1" pin="S0" pad="26"/>
<connect gate="G1" pin="S1" pad="27"/>
<connect gate="G1" pin="S2" pad="28"/>
<connect gate="G1" pin="SYSTICK" pad="23"/>
<connect gate="G2" pin="GND@1" pad="1"/>
<connect gate="G2" pin="GND@2" pad="20"/>
<connect gate="G2" pin="VCC" pad="40"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*257" prefix="IC">
<description>Quadruple 2-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74257"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!A!/B" pad="2"/>
<connect gate="A" pin="1A" pad="3"/>
<connect gate="A" pin="1B" pad="4"/>
<connect gate="A" pin="1Y" pad="5"/>
<connect gate="A" pin="2A" pad="7"/>
<connect gate="A" pin="2B" pad="8"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="12"/>
<connect gate="A" pin="4A" pad="18"/>
<connect gate="A" pin="4B" pad="17"/>
<connect gate="A" pin="4Y" pad="15"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="20X8" prefix="IC" uservalue="yes">
<description>&lt;b&gt;PAL&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="20X8"/>
<gate name="P" symbol="PWRN-2"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="A" pin="!OE" pad="13"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="I2" pad="4"/>
<connect gate="A" pin="I3" pad="5"/>
<connect gate="A" pin="I4" pad="6"/>
<connect gate="A" pin="I5" pad="7"/>
<connect gate="A" pin="I6" pad="8"/>
<connect gate="A" pin="I7" pad="9"/>
<connect gate="A" pin="I8" pad="10"/>
<connect gate="A" pin="I9" pad="11"/>
<connect gate="A" pin="O0" pad="23"/>
<connect gate="A" pin="O1" pad="22"/>
<connect gate="A" pin="O2" pad="21"/>
<connect gate="A" pin="O3" pad="20"/>
<connect gate="A" pin="O4" pad="19"/>
<connect gate="A" pin="O5" pad="18"/>
<connect gate="A" pin="O6" pad="17"/>
<connect gate="A" pin="O7" pad="16"/>
<connect gate="A" pin="O8" pad="15"/>
<connect gate="A" pin="O9" pad="14"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="16R6" prefix="IC" uservalue="yes">
<description>&lt;b&gt;PAL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="16R6"/>
<gate name="P" symbol="PWRN-2"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="I0" pad="2"/>
<connect gate="G$1" pin="I1" pad="3"/>
<connect gate="G$1" pin="I2" pad="4"/>
<connect gate="G$1" pin="I3" pad="5"/>
<connect gate="G$1" pin="I4" pad="6"/>
<connect gate="G$1" pin="I5" pad="7"/>
<connect gate="G$1" pin="I6" pad="8"/>
<connect gate="G$1" pin="I7" pad="9"/>
<connect gate="G$1" pin="O0" pad="12"/>
<connect gate="G$1" pin="O1" pad="13"/>
<connect gate="G$1" pin="O2" pad="14"/>
<connect gate="G$1" pin="O3" pad="15"/>
<connect gate="G$1" pin="O4" pad="16"/>
<connect gate="G$1" pin="O5" pad="17"/>
<connect gate="G$1" pin="O6" pad="18"/>
<connect gate="G$1" pin="O7" pad="19"/>
<connect gate="G$1" pin="OE" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="16R4" prefix="IC" uservalue="yes">
<description>&lt;b&gt;PAL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="16R4"/>
<gate name="P" symbol="PWRN-2"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="I0" pad="2"/>
<connect gate="G$1" pin="I1" pad="3"/>
<connect gate="G$1" pin="I2" pad="4"/>
<connect gate="G$1" pin="I3" pad="5"/>
<connect gate="G$1" pin="I4" pad="6"/>
<connect gate="G$1" pin="I5" pad="7"/>
<connect gate="G$1" pin="I6" pad="8"/>
<connect gate="G$1" pin="I7" pad="9"/>
<connect gate="G$1" pin="O0" pad="12"/>
<connect gate="G$1" pin="O1" pad="13"/>
<connect gate="G$1" pin="O2" pad="14"/>
<connect gate="G$1" pin="O3" pad="15"/>
<connect gate="G$1" pin="O4" pad="16"/>
<connect gate="G$1" pin="O5" pad="17"/>
<connect gate="G$1" pin="O6" pad="18"/>
<connect gate="G$1" pin="O7" pad="19"/>
<connect gate="G$1" pin="OE" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCC" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="VCC" symbol="VCC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*245" prefix="IC">
<description>Octal &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74245"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="DIR" pad="1"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="DIR" pad="1"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="DIR" pad="1"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*166" prefix="IC">
<description>8-bit parallel load &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74166"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="A" pin="CLK" pad="7"/>
<connect gate="A" pin="CLR" pad="9"/>
<connect gate="A" pin="D" pad="5"/>
<connect gate="A" pin="E" pad="10"/>
<connect gate="A" pin="F" pad="11"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="H" pad="14"/>
<connect gate="A" pin="INH" pad="6"/>
<connect gate="A" pin="QH" pad="13"/>
<connect gate="A" pin="SER" pad="1"/>
<connect gate="A" pin="SH/!LD" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="A" pin="CLK" pad="7"/>
<connect gate="A" pin="CLR" pad="9"/>
<connect gate="A" pin="D" pad="5"/>
<connect gate="A" pin="E" pad="10"/>
<connect gate="A" pin="F" pad="11"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="H" pad="14"/>
<connect gate="A" pin="INH" pad="6"/>
<connect gate="A" pin="QH" pad="13"/>
<connect gate="A" pin="SER" pad="1"/>
<connect gate="A" pin="SH/!LD" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="CLR" pad="12"/>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="E" pad="13"/>
<connect gate="A" pin="F" pad="14"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="A" pin="H" pad="18"/>
<connect gate="A" pin="INH" pad="8"/>
<connect gate="A" pin="QH" pad="17"/>
<connect gate="A" pin="SER" pad="2"/>
<connect gate="A" pin="SH/!LD" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*04" prefix="IC">
<description>Hex &lt;b&gt;INVERTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7404"/>
<gate name="B" symbol="7404"/>
<gate name="C" symbol="7404"/>
<gate name="D" symbol="7404"/>
<gate name="E" symbol="7404"/>
<gate name="F" symbol="7404"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I" pad="4"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I" pad="8"/>
<connect gate="C" pin="O" pad="9"/>
<connect gate="D" pin="I" pad="13"/>
<connect gate="D" pin="O" pad="12"/>
<connect gate="E" pin="I" pad="16"/>
<connect gate="E" pin="O" pad="14"/>
<connect gate="F" pin="I" pad="19"/>
<connect gate="F" pin="O" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*08" prefix="IC">
<description>Quad 2-input &lt;b&gt;AND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7408"/>
<gate name="B" symbol="7408"/>
<gate name="C" symbol="7408"/>
<gate name="D" symbol="7408"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="B" pin="I0" pad="6"/>
<connect gate="B" pin="I1" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="D" pin="I0" pad="18"/>
<connect gate="D" pin="I1" pad="19"/>
<connect gate="D" pin="O" pad="16"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*10" prefix="IC">
<description>Triple 3-input &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7410"/>
<gate name="B" symbol="7410"/>
<gate name="C" symbol="7410"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I0" pad="3"/>
<connect gate="B" pin="I1" pad="4"/>
<connect gate="B" pin="I2" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="I2" pad="11"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I0" pad="3"/>
<connect gate="B" pin="I1" pad="4"/>
<connect gate="B" pin="I2" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="I2" pad="11"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="I2" pad="19"/>
<connect gate="A" pin="O" pad="18"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="I2" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="I2" pad="16"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*30" prefix="IC">
<description>8-input &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7430"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="3"/>
<connect gate="A" pin="I3" pad="4"/>
<connect gate="A" pin="I4" pad="5"/>
<connect gate="A" pin="I5" pad="6"/>
<connect gate="A" pin="I6" pad="11"/>
<connect gate="A" pin="I7" pad="12"/>
<connect gate="A" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="3"/>
<connect gate="A" pin="I3" pad="4"/>
<connect gate="A" pin="I4" pad="5"/>
<connect gate="A" pin="I5" pad="6"/>
<connect gate="A" pin="I6" pad="11"/>
<connect gate="A" pin="I7" pad="12"/>
<connect gate="A" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="I2" pad="4"/>
<connect gate="A" pin="I3" pad="6"/>
<connect gate="A" pin="I4" pad="8"/>
<connect gate="A" pin="I5" pad="9"/>
<connect gate="A" pin="I6" pad="16"/>
<connect gate="A" pin="I7" pad="18"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*109" prefix="IC">
<description>Dual J-K positive edge triggered &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset and clear</description>
<gates>
<gate name="A" symbol="74109"/>
<gate name="B" symbol="74109"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!Q" pad="7"/>
<connect gate="A" pin="CLK" pad="4"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="J" pad="2"/>
<connect gate="A" pin="K" pad="3"/>
<connect gate="A" pin="PRE" pad="5"/>
<connect gate="A" pin="Q" pad="6"/>
<connect gate="B" pin="!Q" pad="9"/>
<connect gate="B" pin="CLK" pad="12"/>
<connect gate="B" pin="CLR" pad="15"/>
<connect gate="B" pin="J" pad="14"/>
<connect gate="B" pin="K" pad="13"/>
<connect gate="B" pin="PRE" pad="11"/>
<connect gate="B" pin="Q" pad="10"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!Q" pad="7"/>
<connect gate="A" pin="CLK" pad="4"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="J" pad="2"/>
<connect gate="A" pin="K" pad="3"/>
<connect gate="A" pin="PRE" pad="5"/>
<connect gate="A" pin="Q" pad="6"/>
<connect gate="B" pin="!Q" pad="9"/>
<connect gate="B" pin="CLK" pad="12"/>
<connect gate="B" pin="CLR" pad="15"/>
<connect gate="B" pin="J" pad="14"/>
<connect gate="B" pin="K" pad="13"/>
<connect gate="B" pin="PRE" pad="11"/>
<connect gate="B" pin="Q" pad="10"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!Q" pad="9"/>
<connect gate="A" pin="CLK" pad="5"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="J" pad="3"/>
<connect gate="A" pin="K" pad="4"/>
<connect gate="A" pin="PRE" pad="7"/>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="B" pin="!Q" pad="12"/>
<connect gate="B" pin="CLK" pad="15"/>
<connect gate="B" pin="CLR" pad="19"/>
<connect gate="B" pin="J" pad="18"/>
<connect gate="B" pin="K" pad="17"/>
<connect gate="B" pin="PRE" pad="14"/>
<connect gate="B" pin="Q" pad="13"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*138" prefix="IC">
<description>3-line to 8-line &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74138"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="G1" pad="6"/>
<connect gate="A" pin="G2A" pad="4"/>
<connect gate="A" pin="G2B" pad="5"/>
<connect gate="A" pin="Y0" pad="15"/>
<connect gate="A" pin="Y1" pad="14"/>
<connect gate="A" pin="Y2" pad="13"/>
<connect gate="A" pin="Y3" pad="12"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="9"/>
<connect gate="A" pin="Y7" pad="7"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="G1" pad="6"/>
<connect gate="A" pin="G2A" pad="4"/>
<connect gate="A" pin="G2B" pad="5"/>
<connect gate="A" pin="Y0" pad="15"/>
<connect gate="A" pin="Y1" pad="14"/>
<connect gate="A" pin="Y2" pad="13"/>
<connect gate="A" pin="Y3" pad="12"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="9"/>
<connect gate="A" pin="Y7" pad="7"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="A" pin="G1" pad="8"/>
<connect gate="A" pin="G2A" pad="5"/>
<connect gate="A" pin="G2B" pad="7"/>
<connect gate="A" pin="Y0" pad="19"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="15"/>
<connect gate="A" pin="Y4" pad="14"/>
<connect gate="A" pin="Y5" pad="13"/>
<connect gate="A" pin="Y6" pad="12"/>
<connect gate="A" pin="Y7" pad="9"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*156" prefix="IC">
<description>Dual 2-line to 4-line &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74156"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1C" pad="1"/>
<connect gate="A" pin="1G" pad="2"/>
<connect gate="A" pin="1Y0" pad="7"/>
<connect gate="A" pin="1Y1" pad="6"/>
<connect gate="A" pin="1Y2" pad="5"/>
<connect gate="A" pin="1Y3" pad="4"/>
<connect gate="A" pin="2C" pad="15"/>
<connect gate="A" pin="2G" pad="14"/>
<connect gate="A" pin="2Y0" pad="9"/>
<connect gate="A" pin="2Y1" pad="10"/>
<connect gate="A" pin="2Y2" pad="11"/>
<connect gate="A" pin="2Y3" pad="12"/>
<connect gate="A" pin="A" pad="13"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1C" pad="1"/>
<connect gate="A" pin="1G" pad="2"/>
<connect gate="A" pin="1Y0" pad="7"/>
<connect gate="A" pin="1Y1" pad="6"/>
<connect gate="A" pin="1Y2" pad="5"/>
<connect gate="A" pin="1Y3" pad="4"/>
<connect gate="A" pin="2C" pad="15"/>
<connect gate="A" pin="2G" pad="14"/>
<connect gate="A" pin="2Y0" pad="9"/>
<connect gate="A" pin="2Y1" pad="10"/>
<connect gate="A" pin="2Y2" pad="11"/>
<connect gate="A" pin="2Y3" pad="12"/>
<connect gate="A" pin="A" pad="13"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="1C" pad="2"/>
<connect gate="A" pin="1G" pad="3"/>
<connect gate="A" pin="1Y0" pad="9"/>
<connect gate="A" pin="1Y1" pad="8"/>
<connect gate="A" pin="1Y2" pad="7"/>
<connect gate="A" pin="1Y3" pad="5"/>
<connect gate="A" pin="2C" pad="19"/>
<connect gate="A" pin="2G" pad="18"/>
<connect gate="A" pin="2Y0" pad="12"/>
<connect gate="A" pin="2Y1" pad="13"/>
<connect gate="A" pin="2Y2" pad="14"/>
<connect gate="A" pin="2Y3" pad="15"/>
<connect gate="A" pin="A" pad="17"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*573" prefix="IC">
<description>8-bit D latch &lt;b&gt;BUS DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74573"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1D" pad="2"/>
<connect gate="A" pin="1Q" pad="19"/>
<connect gate="A" pin="2D" pad="3"/>
<connect gate="A" pin="2Q" pad="18"/>
<connect gate="A" pin="3D" pad="4"/>
<connect gate="A" pin="3Q" pad="17"/>
<connect gate="A" pin="4D" pad="5"/>
<connect gate="A" pin="4Q" pad="16"/>
<connect gate="A" pin="5D" pad="6"/>
<connect gate="A" pin="5Q" pad="15"/>
<connect gate="A" pin="6D" pad="7"/>
<connect gate="A" pin="6Q" pad="14"/>
<connect gate="A" pin="7D" pad="8"/>
<connect gate="A" pin="7Q" pad="13"/>
<connect gate="A" pin="8D" pad="9"/>
<connect gate="A" pin="8Q" pad="12"/>
<connect gate="A" pin="C" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="AS"/>
<technology name="HC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8288" prefix="U">
<gates>
<gate name="G$1" symbol="8288"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="!AEN" pad="6"/>
<connect gate="G$1" pin="!AIOWC" pad="12"/>
<connect gate="G$1" pin="!AMWC" pad="8"/>
<connect gate="G$1" pin="!INTA" pad="14"/>
<connect gate="G$1" pin="!IORC" pad="13"/>
<connect gate="G$1" pin="!IOWC" pad="11"/>
<connect gate="G$1" pin="!MRDC" pad="7"/>
<connect gate="G$1" pin="!MWTC" pad="9"/>
<connect gate="G$1" pin="!S0" pad="19"/>
<connect gate="G$1" pin="!S1" pad="3"/>
<connect gate="G$1" pin="!S2" pad="18"/>
<connect gate="G$1" pin="ALE" pad="5"/>
<connect gate="G$1" pin="CEN" pad="15"/>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="DEN" pad="16"/>
<connect gate="G$1" pin="DT/!R" pad="4"/>
<connect gate="G$1" pin="IOB" pad="1"/>
<connect gate="G$1" pin="MCE/!PDEN" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8284" prefix="U">
<gates>
<gate name="G$1" symbol="8284"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="!AEN1" pad="3"/>
<connect gate="G$1" pin="!AEN2" pad="7"/>
<connect gate="G$1" pin="!ASYNC" pad="15"/>
<connect gate="G$1" pin="!RDY1" pad="4"/>
<connect gate="G$1" pin="!RDY2" pad="6"/>
<connect gate="G$1" pin="!RES" pad="11"/>
<connect gate="G$1" pin="CLK" pad="8"/>
<connect gate="G$1" pin="CSYNC" pad="1"/>
<connect gate="G$1" pin="EFI" pad="14"/>
<connect gate="G$1" pin="F/!C" pad="13"/>
<connect gate="G$1" pin="OSC" pad="12"/>
<connect gate="G$1" pin="PCLK" pad="2"/>
<connect gate="G$1" pin="READY" pad="5"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="X1" pad="17"/>
<connect gate="G$1" pin="X2" pad="16"/>
<connect gate="P" pin="GND" pad="9"/>
<connect gate="P" pin="VCC" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7220" prefix="U">
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="G$1" symbol="7220"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!BOOT.EN" pad="32"/>
<connect gate="G$1" pin="!BOOT.SW.EN" pad="30"/>
<connect gate="G$1" pin="!BUS.RD" pad="25"/>
<connect gate="G$1" pin="!CS" pad="21"/>
<connect gate="G$1" pin="!DACK" pad="7"/>
<connect gate="G$1" pin="!DET.ON" pad="28"/>
<connect gate="G$1" pin="!ERR.FLG" pad="27"/>
<connect gate="G$1" pin="!PWR.FAIL" pad="1"/>
<connect gate="G$1" pin="!RD" pad="5"/>
<connect gate="G$1" pin="!REP.EN" pad="33"/>
<connect gate="G$1" pin="!RESET" pad="4"/>
<connect gate="G$1" pin="!RESET.OUT" pad="2"/>
<connect gate="G$1" pin="!SHIFT.CLK" pad="24"/>
<connect gate="G$1" pin="!SWAP.EN" pad="31"/>
<connect gate="G$1" pin="!SYNC" pad="23"/>
<connect gate="G$1" pin="!TM.A" pad="35"/>
<connect gate="G$1" pin="!TM.B" pad="34"/>
<connect gate="G$1" pin="!WAIT" pad="26"/>
<connect gate="G$1" pin="!WR" pad="6"/>
<connect gate="G$1" pin="!X+" pad="39"/>
<connect gate="G$1" pin="!X-" pad="38"/>
<connect gate="G$1" pin="!Y+" pad="37"/>
<connect gate="G$1" pin="!Y-" pad="36"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="C/!D" pad="29"/>
<connect gate="G$1" pin="CLK" pad="3"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="14"/>
<connect gate="G$1" pin="D4" pad="15"/>
<connect gate="G$1" pin="D5" pad="16"/>
<connect gate="G$1" pin="D6" pad="17"/>
<connect gate="G$1" pin="D7" pad="18"/>
<connect gate="G$1" pin="D8" pad="19"/>
<connect gate="G$1" pin="DIO" pad="22"/>
<connect gate="G$1" pin="DRQ" pad="8"/>
<connect gate="G$1" pin="INT" pad="9"/>
<connect gate="P" pin="GND" pad="20"/>
<connect gate="P" pin="VCC" pad="40"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VDD" prefix="VDD">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="VDD"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7230" prefix="U">
<gates>
<gate name="G" symbol="7230"/>
<gate name="P2" symbol="VDD"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL22">
<connects>
<connect gate="G" pin="!BOOT.EN" pad="10"/>
<connect gate="G" pin="!BOOT.SW.EN" pad="9"/>
<connect gate="G" pin="!CS" pad="7"/>
<connect gate="G" pin="!GEN.EN.A" pad="5"/>
<connect gate="G" pin="!GEN.EN.B" pad="4"/>
<connect gate="G" pin="!PWR.FAIL" pad="21"/>
<connect gate="G" pin="!REP.EN" pad="8"/>
<connect gate="G" pin="!SWAP.EN" pad="6"/>
<connect gate="G" pin="!TM.A" pad="2"/>
<connect gate="G" pin="!TM.B" pad="3"/>
<connect gate="G" pin="BOOT.REP" pad="13"/>
<connect gate="G" pin="BOOT.SW" pad="14"/>
<connect gate="G" pin="GEN.A" pad="19"/>
<connect gate="G" pin="GEN.B" pad="18"/>
<connect gate="G" pin="REF.RES" pad="20"/>
<connect gate="G" pin="REP.A" pad="15"/>
<connect gate="G" pin="REP.B" pad="16"/>
<connect gate="G" pin="SWAP" pad="17"/>
<connect gate="P" pin="GND" pad="11 12"/>
<connect gate="P" pin="VCC" pad="22"/>
<connect gate="P2" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7242" prefix="U">
<gates>
<gate name="G" symbol="7242"/>
<gate name="P" symbol="PWRN"/>
<gate name="P2" symbol="VDD"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G" pin="!CS" pad="1"/>
<connect gate="G" pin="!DATA.OUT.A" pad="11"/>
<connect gate="G" pin="!DATA.OUT.B" pad="12"/>
<connect gate="G" pin="!DET.A+" pad="6"/>
<connect gate="G" pin="!DET.A-" pad="7"/>
<connect gate="G" pin="!DET.B+" pad="8"/>
<connect gate="G" pin="!DET.B-" pad="9"/>
<connect gate="G" pin="!ENABLE.A" pad="13"/>
<connect gate="G" pin="!ENABLE.B" pad="14"/>
<connect gate="G" pin="!ERR.FLG" pad="4"/>
<connect gate="G" pin="!RESET" pad="16"/>
<connect gate="G" pin="!SELECT.IN" pad="19"/>
<connect gate="G" pin="!SELECT.OUT" pad="2"/>
<connect gate="G" pin="!SHIFT.CLK" pad="15"/>
<connect gate="G" pin="C/!D" pad="3"/>
<connect gate="G" pin="CLK" pad="18"/>
<connect gate="G" pin="DIO" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
<connect gate="P2" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7250" prefix="U">
<gates>
<gate name="G" symbol="7250"/>
<gate name="P2" symbol="VDD"/>
<gate name="P" symbol="GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G" pin="!CS" pad="1"/>
<connect gate="G" pin="!RESET" pad="2"/>
<connect gate="G" pin="!X+.IN" pad="3"/>
<connect gate="G" pin="!X+.OUT" pad="15"/>
<connect gate="G" pin="!X-.IN" pad="4"/>
<connect gate="G" pin="!X-.OUT" pad="13"/>
<connect gate="G" pin="!Y+.IN" pad="5"/>
<connect gate="G" pin="!Y+.OUT" pad="11"/>
<connect gate="G" pin="!Y-.IN" pad="6"/>
<connect gate="G" pin="!Y-.OUT" pad="9"/>
<connect gate="G" pin="X+.OUT" pad="14"/>
<connect gate="G" pin="X-.OUT" pad="12"/>
<connect gate="G" pin="Y+.OUT" pad="10"/>
<connect gate="G" pin="Y-.OUT" pad="7"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P2" pin="VDD" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7254" prefix="U">
<gates>
<gate name="G$1" symbol="7254"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="D1" pad="1"/>
<connect gate="G$1" pin="D2" pad="7"/>
<connect gate="G$1" pin="D3" pad="8"/>
<connect gate="G$1" pin="D4" pad="14"/>
<connect gate="G$1" pin="G1" pad="3"/>
<connect gate="G$1" pin="G2" pad="5"/>
<connect gate="G$1" pin="G3" pad="10"/>
<connect gate="G$1" pin="G4" pad="12"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="NC1" pad="11"/>
<connect gate="G$1" pin="S1" pad="2"/>
<connect gate="G$1" pin="S2" pad="6"/>
<connect gate="G$1" pin="S3" pad="9"/>
<connect gate="G$1" pin="S4" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7110" prefix="BM">
<gates>
<gate name="G" symbol="7110"/>
</gates>
<devices>
<device name="" package="7110">
<connects>
<connect gate="G" pin="BOOT.REP" pad="4"/>
<connect gate="G" pin="BOOT.SWAP" pad="5"/>
<connect gate="G" pin="DET.COM" pad="15"/>
<connect gate="G" pin="DET.OUT.A+" pad="19"/>
<connect gate="G" pin="DET.OUT.A-" pad="18"/>
<connect gate="G" pin="DET.OUT.B+" pad="17"/>
<connect gate="G" pin="DET.OUT.B-" pad="16"/>
<connect gate="G" pin="DET.SUPPLY" pad="20"/>
<connect gate="G" pin="GENERATE.A" pad="7"/>
<connect gate="G" pin="GENERATE.B" pad="8"/>
<connect gate="G" pin="NC" pad="6"/>
<connect gate="G" pin="PULSE.COM" pad="1"/>
<connect gate="G" pin="REPLICATE.A" pad="3"/>
<connect gate="G" pin="REPLICATE.B" pad="2"/>
<connect gate="G" pin="SWAP.A" pad="13"/>
<connect gate="G" pin="SWAP.B" pad="14"/>
<connect gate="G" pin="X+.COIL.IN" pad="10"/>
<connect gate="G" pin="X-.COIL.IN" pad="9"/>
<connect gate="G" pin="Y+.COIL.IN" pad="12"/>
<connect gate="G" pin="Y-.COIL.IN" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN75453B" prefix="IC">
<description>&lt;b&gt;OR&lt;/b&gt; PERIPHERAL DRIVERS FOR HIGH-CURRENT SWITCHING AT VERY HIGH SPEEDS&lt;p&gt;
Source: www.ti.com sn75452b.pdf</description>
<gates>
<gate name="A" symbol="OR"/>
<gate name="B" symbol="OR"/>
<gate name="P" symbol="PWRN-3"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="7"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="5"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="JG" package="DIL08">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="7"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="5"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="D_R-PDSO-G8">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="7"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="5"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PS" package="PS_R-PDSO-G8">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="7"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="5"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN75160BDW" prefix="U">
<description>TRANSCEIVER</description>
<gates>
<gate name="A" symbol="SN75160BDW"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-20N">
<connects>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="3"/>
<connect gate="A" pin="B3" pad="4"/>
<connect gate="A" pin="B4" pad="5"/>
<connect gate="A" pin="B5" pad="6"/>
<connect gate="A" pin="B6" pad="7"/>
<connect gate="A" pin="B7" pad="8"/>
<connect gate="A" pin="B8" pad="9"/>
<connect gate="A" pin="D1" pad="19"/>
<connect gate="A" pin="D2" pad="18"/>
<connect gate="A" pin="D3" pad="17"/>
<connect gate="A" pin="D4" pad="16"/>
<connect gate="A" pin="D5" pad="15"/>
<connect gate="A" pin="D6" pad="14"/>
<connect gate="A" pin="D7" pad="13"/>
<connect gate="A" pin="D8" pad="12"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="PE" pad="11"/>
<connect gate="A" pin="TE" pad="1"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SN75160BDW"/>
<attribute name="OC_FARNELL" value="1470454"/>
<attribute name="OC_NEWARK" value="67K2870"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="TEXAS INSTRUMENTS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN75160BDWR" prefix="U">
<description>OCTAL GENERAL-PURPOSE INTERFACE BUS TRANSCEIVER</description>
<gates>
<gate name="A" symbol="SN75160BDWR"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-20N">
<connects>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="3"/>
<connect gate="A" pin="B3" pad="4"/>
<connect gate="A" pin="B4" pad="5"/>
<connect gate="A" pin="B5" pad="6"/>
<connect gate="A" pin="B6" pad="7"/>
<connect gate="A" pin="B7" pad="8"/>
<connect gate="A" pin="B8" pad="9"/>
<connect gate="A" pin="D1" pad="19"/>
<connect gate="A" pin="D2" pad="18"/>
<connect gate="A" pin="D3" pad="17"/>
<connect gate="A" pin="D4" pad="16"/>
<connect gate="A" pin="D5" pad="15"/>
<connect gate="A" pin="D6" pad="14"/>
<connect gate="A" pin="D7" pad="13"/>
<connect gate="A" pin="D8" pad="12"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="PE" pad="11"/>
<connect gate="A" pin="TE" pad="1"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SN75160BDWR"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="76C5346"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN75160BN" prefix="U">
<description>OCTAL GENERAL-PURPOSE INTERFACE BUS TRANSCEIVER</description>
<gates>
<gate name="A" symbol="SN75160BN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-20">
<connects>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="3"/>
<connect gate="A" pin="B3" pad="4"/>
<connect gate="A" pin="B4" pad="5"/>
<connect gate="A" pin="B5" pad="6"/>
<connect gate="A" pin="B6" pad="7"/>
<connect gate="A" pin="B7" pad="8"/>
<connect gate="A" pin="B8" pad="9"/>
<connect gate="A" pin="D1" pad="19"/>
<connect gate="A" pin="D2" pad="18"/>
<connect gate="A" pin="D3" pad="17"/>
<connect gate="A" pin="D4" pad="16"/>
<connect gate="A" pin="D5" pad="15"/>
<connect gate="A" pin="D6" pad="14"/>
<connect gate="A" pin="D7" pad="13"/>
<connect gate="A" pin="D8" pad="12"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="PE" pad="11"/>
<connect gate="A" pin="TE" pad="1"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SN75160BN"/>
<attribute name="OC_FARNELL" value="1470448"/>
<attribute name="OC_NEWARK" value="60K6925"/>
<attribute name="PACKAGE" value="PDIP-20"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN75161BDW" prefix="U">
<description>OCTAL GENERAL-PURPOSE INTERFACE BUS TRANSCEIVERS</description>
<gates>
<gate name="A" symbol="SN75161BDW"/>
</gates>
<devices>
<device name="" package="SOIC127P1032X265-20N">
<connects>
<connect gate="A" pin="ATN" pad="8"/>
<connect gate="A" pin="ATN_2" pad="13"/>
<connect gate="A" pin="DAV" pad="6"/>
<connect gate="A" pin="DAV_2" pad="15"/>
<connect gate="A" pin="DC" pad="11"/>
<connect gate="A" pin="EOI" pad="7"/>
<connect gate="A" pin="EOI_2" pad="14"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="IFC" pad="3"/>
<connect gate="A" pin="IFC_2" pad="18"/>
<connect gate="A" pin="NDAC" pad="4"/>
<connect gate="A" pin="NDAC_2" pad="17"/>
<connect gate="A" pin="NRFD" pad="5"/>
<connect gate="A" pin="NRFD_2" pad="16"/>
<connect gate="A" pin="REN" pad="19"/>
<connect gate="A" pin="REN_2" pad="2"/>
<connect gate="A" pin="SRQ" pad="12"/>
<connect gate="A" pin="SRQ_2" pad="9"/>
<connect gate="A" pin="TE" pad="1"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SN75161BDW"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="OC_NEWARK" value="08F8092"/>
<attribute name="PACKAGE" value="SOIC-20"/>
<attribute name="SUPPLIER" value="TEXAS INSTRUMENTS"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN75161BN" prefix="U">
<description>OCTAL GENERAL-PURPOSE INTERFACE BUS TRANSCEIVERS</description>
<gates>
<gate name="A" symbol="SN75161BN"/>
</gates>
<devices>
<device name="" package="DIP254P762X508-20">
<connects>
<connect gate="A" pin="ATN" pad="13"/>
<connect gate="A" pin="ATN_2" pad="8"/>
<connect gate="A" pin="DAV" pad="15"/>
<connect gate="A" pin="DAV_2" pad="6"/>
<connect gate="A" pin="DC" pad="11"/>
<connect gate="A" pin="EOI" pad="14"/>
<connect gate="A" pin="EOI_2" pad="7"/>
<connect gate="A" pin="GND" pad="10"/>
<connect gate="A" pin="IFC" pad="18"/>
<connect gate="A" pin="IFC_2" pad="3"/>
<connect gate="A" pin="NDAC" pad="17"/>
<connect gate="A" pin="NDAC_2" pad="4"/>
<connect gate="A" pin="NRFD" pad="16"/>
<connect gate="A" pin="NRFD_2" pad="5"/>
<connect gate="A" pin="REN" pad="19"/>
<connect gate="A" pin="REN_2" pad="2"/>
<connect gate="A" pin="SRQ" pad="12"/>
<connect gate="A" pin="SRQ_2" pad="9"/>
<connect gate="A" pin="TE" pad="1"/>
<connect gate="A" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SN75161BN"/>
<attribute name="OC_FARNELL" value="1470452"/>
<attribute name="OC_NEWARK" value="62K3469"/>
<attribute name="PACKAGE" value="PDIP-20"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN75162BDW" prefix="U">
<description>OCTAL GENERAL-PURPOSE INTERFACE BUS TRANSCEIVERS</description>
<gates>
<gate name="A" symbol="SN75162BDW"/>
</gates>
<devices>
<device name="" package="SOIC127P1030X265-24N">
<connects>
<connect gate="A" pin="ATN" pad="16"/>
<connect gate="A" pin="ATN_2" pad="9"/>
<connect gate="A" pin="DAV" pad="18"/>
<connect gate="A" pin="DAV_2" pad="7"/>
<connect gate="A" pin="DC" pad="13"/>
<connect gate="A" pin="EOI" pad="8"/>
<connect gate="A" pin="EOI_2" pad="17"/>
<connect gate="A" pin="GND" pad="12"/>
<connect gate="A" pin="IFC" pad="21"/>
<connect gate="A" pin="IFC_2" pad="4"/>
<connect gate="A" pin="NC" pad="11"/>
<connect gate="A" pin="NC_2" pad="23"/>
<connect gate="A" pin="NC_3" pad="14"/>
<connect gate="A" pin="NDAC" pad="20"/>
<connect gate="A" pin="NDAC_2" pad="5"/>
<connect gate="A" pin="NRFD" pad="19"/>
<connect gate="A" pin="NRFD_2" pad="6"/>
<connect gate="A" pin="REN" pad="22"/>
<connect gate="A" pin="REN_2" pad="3"/>
<connect gate="A" pin="SC" pad="1"/>
<connect gate="A" pin="SRQ" pad="15"/>
<connect gate="A" pin="SRQ_2" pad="10"/>
<connect gate="A" pin="TE" pad="2"/>
<connect gate="A" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SN75162BDW"/>
<attribute name="OC_FARNELL" value="3583454"/>
<attribute name="OC_NEWARK" value="08F8095"/>
<attribute name="PACKAGE" value="SOIC-24"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C24HP" prefix="PL" uservalue="yes">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="24G"/>
</gates>
<devices>
<device name="" package="24HP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="G1" pad="G1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GPIB-PINHD-2X12" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="GPIB-PINHD-2X12"/>
</gates>
<devices>
<device name="" package="GPIB-PINHD-2X12">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="GPIB-PINHD-2X12/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPBERRY-PI+">
<description>Samtec SSW-120-01-T-D</description>
<gates>
<gate name="G$1" symbol="RASPBERRY-PI+"/>
</gates>
<devices>
<device name="" package="RASPBERRY-PI-PLUS-CAM_NOTCH">
<connects>
<connect gate="G$1" pin="1-3V3" pad="P$1"/>
<connect gate="G$1" pin="10-RX" pad="P$10"/>
<connect gate="G$1" pin="11-GPIO17" pad="P$11"/>
<connect gate="G$1" pin="12-GPIO18" pad="P$12"/>
<connect gate="G$1" pin="13-GPIO27" pad="P$13"/>
<connect gate="G$1" pin="14-GND" pad="P$14"/>
<connect gate="G$1" pin="15-GPIO22" pad="P$15"/>
<connect gate="G$1" pin="16-GPIO23" pad="P$16"/>
<connect gate="G$1" pin="17-3V3" pad="P$17"/>
<connect gate="G$1" pin="18-GPIO24" pad="P$18"/>
<connect gate="G$1" pin="19-SPI-MOSI/GPIO10" pad="P$19"/>
<connect gate="G$1" pin="2-5V" pad="P$2"/>
<connect gate="G$1" pin="20-GND" pad="P$20"/>
<connect gate="G$1" pin="21-SPI-MISO/GPIO9" pad="P$21"/>
<connect gate="G$1" pin="22-GPIO25" pad="P$22"/>
<connect gate="G$1" pin="23-SPI-SCLK/GPIO11" pad="P$23"/>
<connect gate="G$1" pin="24-GPIO8" pad="P$24"/>
<connect gate="G$1" pin="25-GND" pad="P$25"/>
<connect gate="G$1" pin="26-GPIO7" pad="P$26"/>
<connect gate="G$1" pin="27-ID_SD" pad="P$27"/>
<connect gate="G$1" pin="28-ID_SC" pad="P$28"/>
<connect gate="G$1" pin="29-GPIO5" pad="P$29"/>
<connect gate="G$1" pin="3-SDA1/GPIO2" pad="P$3"/>
<connect gate="G$1" pin="30-GND" pad="P$30"/>
<connect gate="G$1" pin="31-GPIO6" pad="P$31"/>
<connect gate="G$1" pin="32-GPIO12" pad="P$32"/>
<connect gate="G$1" pin="33-GPIO13" pad="P$33"/>
<connect gate="G$1" pin="34-GND" pad="P$34"/>
<connect gate="G$1" pin="35-GPIO19" pad="P$35"/>
<connect gate="G$1" pin="36-GPIO16" pad="P$36"/>
<connect gate="G$1" pin="37-GPIO26" pad="P$37"/>
<connect gate="G$1" pin="38-GPIO20" pad="P$38"/>
<connect gate="G$1" pin="39-GND" pad="P$39"/>
<connect gate="G$1" pin="4-5V" pad="P$4"/>
<connect gate="G$1" pin="40-GPIO21" pad="P$40"/>
<connect gate="G$1" pin="5-SCL1/GPIO3" pad="P$5"/>
<connect gate="G$1" pin="6-GND" pad="P$6"/>
<connect gate="G$1" pin="7-GPIO4" pad="P$7"/>
<connect gate="G$1" pin="8-TX" pad="P$8"/>
<connect gate="G$1" pin="9-GND" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NONOTCHES" package="RASPBERRY-PI-PLUS">
<connects>
<connect gate="G$1" pin="1-3V3" pad="1"/>
<connect gate="G$1" pin="10-RX" pad="10"/>
<connect gate="G$1" pin="11-GPIO17" pad="11"/>
<connect gate="G$1" pin="12-GPIO18" pad="12"/>
<connect gate="G$1" pin="13-GPIO27" pad="13"/>
<connect gate="G$1" pin="14-GND" pad="14"/>
<connect gate="G$1" pin="15-GPIO22" pad="15"/>
<connect gate="G$1" pin="16-GPIO23" pad="16"/>
<connect gate="G$1" pin="17-3V3" pad="17"/>
<connect gate="G$1" pin="18-GPIO24" pad="18"/>
<connect gate="G$1" pin="19-SPI-MOSI/GPIO10" pad="19"/>
<connect gate="G$1" pin="2-5V" pad="2"/>
<connect gate="G$1" pin="20-GND" pad="20"/>
<connect gate="G$1" pin="21-SPI-MISO/GPIO9" pad="21"/>
<connect gate="G$1" pin="22-GPIO25" pad="22"/>
<connect gate="G$1" pin="23-SPI-SCLK/GPIO11" pad="23"/>
<connect gate="G$1" pin="24-GPIO8" pad="24"/>
<connect gate="G$1" pin="25-GND" pad="25"/>
<connect gate="G$1" pin="26-GPIO7" pad="26"/>
<connect gate="G$1" pin="27-ID_SD" pad="27"/>
<connect gate="G$1" pin="28-ID_SC" pad="28"/>
<connect gate="G$1" pin="29-GPIO5" pad="29"/>
<connect gate="G$1" pin="3-SDA1/GPIO2" pad="3"/>
<connect gate="G$1" pin="30-GND" pad="30"/>
<connect gate="G$1" pin="31-GPIO6" pad="31"/>
<connect gate="G$1" pin="32-GPIO12" pad="32"/>
<connect gate="G$1" pin="33-GPIO13" pad="33"/>
<connect gate="G$1" pin="34-GND" pad="34"/>
<connect gate="G$1" pin="35-GPIO19" pad="35"/>
<connect gate="G$1" pin="36-GPIO16" pad="36"/>
<connect gate="G$1" pin="37-GPIO26" pad="37"/>
<connect gate="G$1" pin="38-GPIO20" pad="38"/>
<connect gate="G$1" pin="39-GND" pad="39"/>
<connect gate="G$1" pin="4-5V" pad="4"/>
<connect gate="G$1" pin="40-GPIO21" pad="40"/>
<connect gate="G$1" pin="5-SCL1/GPIO3" pad="5"/>
<connect gate="G$1" pin="6-GND" pad="6"/>
<connect gate="G$1" pin="7-GPIO4" pad="7"/>
<connect gate="G$1" pin="8-TX" pad="8"/>
<connect gate="G$1" pin="9-GND" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CAM/DISPLAY_NOTCH" package="RASPBERRY-PI-PLUS-DISPLAY/CAM_NOTCH">
<connects>
<connect gate="G$1" pin="1-3V3" pad="P$1"/>
<connect gate="G$1" pin="10-RX" pad="P$10"/>
<connect gate="G$1" pin="11-GPIO17" pad="P$11"/>
<connect gate="G$1" pin="12-GPIO18" pad="P$12"/>
<connect gate="G$1" pin="13-GPIO27" pad="P$13"/>
<connect gate="G$1" pin="14-GND" pad="P$14"/>
<connect gate="G$1" pin="15-GPIO22" pad="P$15"/>
<connect gate="G$1" pin="16-GPIO23" pad="P$16"/>
<connect gate="G$1" pin="17-3V3" pad="P$17"/>
<connect gate="G$1" pin="18-GPIO24" pad="P$18"/>
<connect gate="G$1" pin="19-SPI-MOSI/GPIO10" pad="P$19"/>
<connect gate="G$1" pin="2-5V" pad="P$2"/>
<connect gate="G$1" pin="20-GND" pad="P$20"/>
<connect gate="G$1" pin="21-SPI-MISO/GPIO9" pad="P$21"/>
<connect gate="G$1" pin="22-GPIO25" pad="P$22"/>
<connect gate="G$1" pin="23-SPI-SCLK/GPIO11" pad="P$23"/>
<connect gate="G$1" pin="24-GPIO8" pad="P$24"/>
<connect gate="G$1" pin="25-GND" pad="P$25"/>
<connect gate="G$1" pin="26-GPIO7" pad="P$26"/>
<connect gate="G$1" pin="27-ID_SD" pad="P$27"/>
<connect gate="G$1" pin="28-ID_SC" pad="P$28"/>
<connect gate="G$1" pin="29-GPIO5" pad="P$29"/>
<connect gate="G$1" pin="3-SDA1/GPIO2" pad="P$3"/>
<connect gate="G$1" pin="30-GND" pad="P$30"/>
<connect gate="G$1" pin="31-GPIO6" pad="P$31"/>
<connect gate="G$1" pin="32-GPIO12" pad="P$32"/>
<connect gate="G$1" pin="33-GPIO13" pad="P$33"/>
<connect gate="G$1" pin="34-GND" pad="P$34"/>
<connect gate="G$1" pin="35-GPIO19" pad="P$35"/>
<connect gate="G$1" pin="36-GPIO16" pad="P$36"/>
<connect gate="G$1" pin="37-GPIO26" pad="P$37"/>
<connect gate="G$1" pin="38-GPIO20" pad="P$38"/>
<connect gate="G$1" pin="39-GND" pad="P$39"/>
<connect gate="G$1" pin="4-5V" pad="P$4"/>
<connect gate="G$1" pin="40-GPIO21" pad="P$40"/>
<connect gate="G$1" pin="5-SCL1/GPIO3" pad="P$5"/>
<connect gate="G$1" pin="6-GND" pad="P$6"/>
<connect gate="G$1" pin="7-GPIO4" pad="P$7"/>
<connect gate="G$1" pin="8-TX" pad="P$8"/>
<connect gate="G$1" pin="9-GND" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RASPBERRY-PI-PLUS-NOOUTLINE" package="RASPBERRY-PI-PLUS-NOOUTLINE">
<connects>
<connect gate="G$1" pin="1-3V3" pad="1"/>
<connect gate="G$1" pin="10-RX" pad="10"/>
<connect gate="G$1" pin="11-GPIO17" pad="11"/>
<connect gate="G$1" pin="12-GPIO18" pad="12"/>
<connect gate="G$1" pin="13-GPIO27" pad="13"/>
<connect gate="G$1" pin="14-GND" pad="14"/>
<connect gate="G$1" pin="15-GPIO22" pad="15"/>
<connect gate="G$1" pin="16-GPIO23" pad="16"/>
<connect gate="G$1" pin="17-3V3" pad="17"/>
<connect gate="G$1" pin="18-GPIO24" pad="18"/>
<connect gate="G$1" pin="19-SPI-MOSI/GPIO10" pad="19"/>
<connect gate="G$1" pin="2-5V" pad="2"/>
<connect gate="G$1" pin="20-GND" pad="20"/>
<connect gate="G$1" pin="21-SPI-MISO/GPIO9" pad="21"/>
<connect gate="G$1" pin="22-GPIO25" pad="22"/>
<connect gate="G$1" pin="23-SPI-SCLK/GPIO11" pad="23"/>
<connect gate="G$1" pin="24-GPIO8" pad="24"/>
<connect gate="G$1" pin="25-GND" pad="25"/>
<connect gate="G$1" pin="26-GPIO7" pad="26"/>
<connect gate="G$1" pin="27-ID_SD" pad="27"/>
<connect gate="G$1" pin="28-ID_SC" pad="28"/>
<connect gate="G$1" pin="29-GPIO5" pad="29"/>
<connect gate="G$1" pin="3-SDA1/GPIO2" pad="3"/>
<connect gate="G$1" pin="30-GND" pad="30"/>
<connect gate="G$1" pin="31-GPIO6" pad="31"/>
<connect gate="G$1" pin="32-GPIO12" pad="32"/>
<connect gate="G$1" pin="33-GPIO13" pad="33"/>
<connect gate="G$1" pin="34-GND" pad="34"/>
<connect gate="G$1" pin="35-GPIO19" pad="35"/>
<connect gate="G$1" pin="36-GPIO16" pad="36"/>
<connect gate="G$1" pin="37-GPIO26" pad="37"/>
<connect gate="G$1" pin="38-GPIO20" pad="38"/>
<connect gate="G$1" pin="39-GND" pad="39"/>
<connect gate="G$1" pin="4-5V" pad="4"/>
<connect gate="G$1" pin="40-GPIO21" pad="40"/>
<connect gate="G$1" pin="5-SCL1/GPIO3" pad="5"/>
<connect gate="G$1" pin="6-GND" pad="6"/>
<connect gate="G$1" pin="7-GPIO4" pad="7"/>
<connect gate="G$1" pin="8-TX" pad="8"/>
<connect gate="G$1" pin="9-GND" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HEADERONLY" package="RASPBERRY-PI-PLUS-HEADERONLY">
<connects>
<connect gate="G$1" pin="1-3V3" pad="1"/>
<connect gate="G$1" pin="10-RX" pad="10"/>
<connect gate="G$1" pin="11-GPIO17" pad="11"/>
<connect gate="G$1" pin="12-GPIO18" pad="12"/>
<connect gate="G$1" pin="13-GPIO27" pad="13"/>
<connect gate="G$1" pin="14-GND" pad="14"/>
<connect gate="G$1" pin="15-GPIO22" pad="15"/>
<connect gate="G$1" pin="16-GPIO23" pad="16"/>
<connect gate="G$1" pin="17-3V3" pad="17"/>
<connect gate="G$1" pin="18-GPIO24" pad="18"/>
<connect gate="G$1" pin="19-SPI-MOSI/GPIO10" pad="19"/>
<connect gate="G$1" pin="2-5V" pad="2"/>
<connect gate="G$1" pin="20-GND" pad="20"/>
<connect gate="G$1" pin="21-SPI-MISO/GPIO9" pad="21"/>
<connect gate="G$1" pin="22-GPIO25" pad="22"/>
<connect gate="G$1" pin="23-SPI-SCLK/GPIO11" pad="23"/>
<connect gate="G$1" pin="24-GPIO8" pad="24"/>
<connect gate="G$1" pin="25-GND" pad="25"/>
<connect gate="G$1" pin="26-GPIO7" pad="26"/>
<connect gate="G$1" pin="27-ID_SD" pad="27"/>
<connect gate="G$1" pin="28-ID_SC" pad="28"/>
<connect gate="G$1" pin="29-GPIO5" pad="29"/>
<connect gate="G$1" pin="3-SDA1/GPIO2" pad="3"/>
<connect gate="G$1" pin="30-GND" pad="30"/>
<connect gate="G$1" pin="31-GPIO6" pad="31"/>
<connect gate="G$1" pin="32-GPIO12" pad="32"/>
<connect gate="G$1" pin="33-GPIO13" pad="33"/>
<connect gate="G$1" pin="34-GND" pad="34"/>
<connect gate="G$1" pin="35-GPIO19" pad="35"/>
<connect gate="G$1" pin="36-GPIO16" pad="36"/>
<connect gate="G$1" pin="37-GPIO26" pad="37"/>
<connect gate="G$1" pin="38-GPIO20" pad="38"/>
<connect gate="G$1" pin="39-GND" pad="39"/>
<connect gate="G$1" pin="4-5V" pad="4"/>
<connect gate="G$1" pin="40-GPIO21" pad="40"/>
<connect gate="G$1" pin="5-SCL1/GPIO3" pad="5"/>
<connect gate="G$1" pin="6-GND" pad="6"/>
<connect gate="G$1" pin="7-GPIO4" pad="7"/>
<connect gate="G$1" pin="8-TX" pad="8"/>
<connect gate="G$1" pin="9-GND" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PIZERO" package="RASPBERRY-PI-ZERO">
<connects>
<connect gate="G$1" pin="1-3V3" pad="1"/>
<connect gate="G$1" pin="10-RX" pad="10"/>
<connect gate="G$1" pin="11-GPIO17" pad="11"/>
<connect gate="G$1" pin="12-GPIO18" pad="12"/>
<connect gate="G$1" pin="13-GPIO27" pad="13"/>
<connect gate="G$1" pin="14-GND" pad="14"/>
<connect gate="G$1" pin="15-GPIO22" pad="15"/>
<connect gate="G$1" pin="16-GPIO23" pad="16"/>
<connect gate="G$1" pin="17-3V3" pad="17"/>
<connect gate="G$1" pin="18-GPIO24" pad="18"/>
<connect gate="G$1" pin="19-SPI-MOSI/GPIO10" pad="19"/>
<connect gate="G$1" pin="2-5V" pad="2"/>
<connect gate="G$1" pin="20-GND" pad="20"/>
<connect gate="G$1" pin="21-SPI-MISO/GPIO9" pad="21"/>
<connect gate="G$1" pin="22-GPIO25" pad="22"/>
<connect gate="G$1" pin="23-SPI-SCLK/GPIO11" pad="23"/>
<connect gate="G$1" pin="24-GPIO8" pad="24"/>
<connect gate="G$1" pin="25-GND" pad="25"/>
<connect gate="G$1" pin="26-GPIO7" pad="26"/>
<connect gate="G$1" pin="27-ID_SD" pad="27"/>
<connect gate="G$1" pin="28-ID_SC" pad="28"/>
<connect gate="G$1" pin="29-GPIO5" pad="29"/>
<connect gate="G$1" pin="3-SDA1/GPIO2" pad="3"/>
<connect gate="G$1" pin="30-GND" pad="30"/>
<connect gate="G$1" pin="31-GPIO6" pad="31"/>
<connect gate="G$1" pin="32-GPIO12" pad="32"/>
<connect gate="G$1" pin="33-GPIO13" pad="33"/>
<connect gate="G$1" pin="34-GND" pad="34"/>
<connect gate="G$1" pin="35-GPIO19" pad="35"/>
<connect gate="G$1" pin="36-GPIO16" pad="36"/>
<connect gate="G$1" pin="37-GPIO26" pad="37"/>
<connect gate="G$1" pin="38-GPIO20" pad="38"/>
<connect gate="G$1" pin="39-GND" pad="39"/>
<connect gate="G$1" pin="4-5V" pad="4"/>
<connect gate="G$1" pin="40-GPIO21" pad="40"/>
<connect gate="G$1" pin="5-SCL1/GPIO3" pad="5"/>
<connect gate="G$1" pin="6-GND" pad="6"/>
<connect gate="G$1" pin="7-GPIO4" pad="7"/>
<connect gate="G$1" pin="8-TX" pad="8"/>
<connect gate="G$1" pin="9-GND" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PIZERO-REFLOWHEADER" package="RASPBERRY-PI-ZERO-REFLOWHEADER">
<connects>
<connect gate="G$1" pin="1-3V3" pad="P$1"/>
<connect gate="G$1" pin="10-RX" pad="P$10"/>
<connect gate="G$1" pin="11-GPIO17" pad="P$11"/>
<connect gate="G$1" pin="12-GPIO18" pad="P$12"/>
<connect gate="G$1" pin="13-GPIO27" pad="P$13"/>
<connect gate="G$1" pin="14-GND" pad="P$14"/>
<connect gate="G$1" pin="15-GPIO22" pad="P$15"/>
<connect gate="G$1" pin="16-GPIO23" pad="P$16"/>
<connect gate="G$1" pin="17-3V3" pad="P$17"/>
<connect gate="G$1" pin="18-GPIO24" pad="P$18"/>
<connect gate="G$1" pin="19-SPI-MOSI/GPIO10" pad="P$19"/>
<connect gate="G$1" pin="2-5V" pad="P$2"/>
<connect gate="G$1" pin="20-GND" pad="P$20"/>
<connect gate="G$1" pin="21-SPI-MISO/GPIO9" pad="P$21"/>
<connect gate="G$1" pin="22-GPIO25" pad="P$22"/>
<connect gate="G$1" pin="23-SPI-SCLK/GPIO11" pad="P$23"/>
<connect gate="G$1" pin="24-GPIO8" pad="P$24"/>
<connect gate="G$1" pin="25-GND" pad="P$25"/>
<connect gate="G$1" pin="26-GPIO7" pad="P$26"/>
<connect gate="G$1" pin="27-ID_SD" pad="P$27"/>
<connect gate="G$1" pin="28-ID_SC" pad="P$28"/>
<connect gate="G$1" pin="29-GPIO5" pad="P$29"/>
<connect gate="G$1" pin="3-SDA1/GPIO2" pad="P$3"/>
<connect gate="G$1" pin="30-GND" pad="P$30"/>
<connect gate="G$1" pin="31-GPIO6" pad="P$31"/>
<connect gate="G$1" pin="32-GPIO12" pad="P$32"/>
<connect gate="G$1" pin="33-GPIO13" pad="P$33"/>
<connect gate="G$1" pin="34-GND" pad="P$34"/>
<connect gate="G$1" pin="35-GPIO19" pad="P$35"/>
<connect gate="G$1" pin="36-GPIO16" pad="P$36"/>
<connect gate="G$1" pin="37-GPIO26" pad="P$37"/>
<connect gate="G$1" pin="38-GPIO20" pad="P$38"/>
<connect gate="G$1" pin="39-GND" pad="P$39"/>
<connect gate="G$1" pin="4-5V" pad="P$4"/>
<connect gate="G$1" pin="40-GPIO21" pad="P$40"/>
<connect gate="G$1" pin="5-SCL1/GPIO3" pad="P$5"/>
<connect gate="G$1" pin="6-GND" pad="P$6"/>
<connect gate="G$1" pin="7-GPIO4" pad="P$7"/>
<connect gate="G$1" pin="8-TX" pad="P$8"/>
<connect gate="G$1" pin="9-GND" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CORRECT-HEADER" package="2X20">
<connects>
<connect gate="G$1" pin="1-3V3" pad="1"/>
<connect gate="G$1" pin="10-RX" pad="10"/>
<connect gate="G$1" pin="11-GPIO17" pad="11"/>
<connect gate="G$1" pin="12-GPIO18" pad="12"/>
<connect gate="G$1" pin="13-GPIO27" pad="13"/>
<connect gate="G$1" pin="14-GND" pad="14"/>
<connect gate="G$1" pin="15-GPIO22" pad="15"/>
<connect gate="G$1" pin="16-GPIO23" pad="16"/>
<connect gate="G$1" pin="17-3V3" pad="17"/>
<connect gate="G$1" pin="18-GPIO24" pad="18"/>
<connect gate="G$1" pin="19-SPI-MOSI/GPIO10" pad="19"/>
<connect gate="G$1" pin="2-5V" pad="2"/>
<connect gate="G$1" pin="20-GND" pad="20"/>
<connect gate="G$1" pin="21-SPI-MISO/GPIO9" pad="21"/>
<connect gate="G$1" pin="22-GPIO25" pad="22"/>
<connect gate="G$1" pin="23-SPI-SCLK/GPIO11" pad="23"/>
<connect gate="G$1" pin="24-GPIO8" pad="24"/>
<connect gate="G$1" pin="25-GND" pad="25"/>
<connect gate="G$1" pin="26-GPIO7" pad="26"/>
<connect gate="G$1" pin="27-ID_SD" pad="27"/>
<connect gate="G$1" pin="28-ID_SC" pad="28"/>
<connect gate="G$1" pin="29-GPIO5" pad="29"/>
<connect gate="G$1" pin="3-SDA1/GPIO2" pad="3"/>
<connect gate="G$1" pin="30-GND" pad="30"/>
<connect gate="G$1" pin="31-GPIO6" pad="31"/>
<connect gate="G$1" pin="32-GPIO12" pad="32"/>
<connect gate="G$1" pin="33-GPIO13" pad="33"/>
<connect gate="G$1" pin="34-GND" pad="34"/>
<connect gate="G$1" pin="35-GPIO19" pad="35"/>
<connect gate="G$1" pin="36-GPIO16" pad="36"/>
<connect gate="G$1" pin="37-GPIO26" pad="37"/>
<connect gate="G$1" pin="38-GPIO20" pad="38"/>
<connect gate="G$1" pin="39-GND" pad="39"/>
<connect gate="G$1" pin="4-5V" pad="4"/>
<connect gate="G$1" pin="40-GPIO21" pad="40"/>
<connect gate="G$1" pin="5-SCL1/GPIO3" pad="5"/>
<connect gate="G$1" pin="6-GND" pad="6"/>
<connect gate="G$1" pin="7-GPIO4" pad="7"/>
<connect gate="G$1" pin="8-TX" pad="8"/>
<connect gate="G$1" pin="9-GND" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2764" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2764"/>
<gate name="P" symbol="PWRN-4"/>
</gates>
<devices>
<device name="" package="DIL28">
<connects>
<connect gate="A" pin="!CE" pad="20"/>
<connect gate="A" pin="!OE" pad="22"/>
<connect gate="A" pin="!PGM" pad="27"/>
<connect gate="A" pin="A0" pad="10"/>
<connect gate="A" pin="A1" pad="9"/>
<connect gate="A" pin="A10" pad="21"/>
<connect gate="A" pin="A11" pad="23"/>
<connect gate="A" pin="A12" pad="2"/>
<connect gate="A" pin="A2" pad="8"/>
<connect gate="A" pin="A3" pad="7"/>
<connect gate="A" pin="A4" pad="6"/>
<connect gate="A" pin="A5" pad="5"/>
<connect gate="A" pin="A6" pad="4"/>
<connect gate="A" pin="A7" pad="3"/>
<connect gate="A" pin="A8" pad="25"/>
<connect gate="A" pin="A9" pad="24"/>
<connect gate="A" pin="O0" pad="11"/>
<connect gate="A" pin="O1" pad="12"/>
<connect gate="A" pin="O2" pad="13"/>
<connect gate="A" pin="O3" pad="15"/>
<connect gate="A" pin="O4" pad="16"/>
<connect gate="A" pin="O5" pad="17"/>
<connect gate="A" pin="O6" pad="18"/>
<connect gate="A" pin="O7" pad="19"/>
<connect gate="A" pin="VPP" pad="1"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RN4_PARALLEL">
<gates>
<gate name="RN" symbol="RN4"/>
</gates>
<devices>
<device name="RN" package="RN-8">
<connects>
<connect gate="RN" pin="1" pad="1"/>
<connect gate="RN" pin="2" pad="3"/>
<connect gate="RN" pin="3" pad="5"/>
<connect gate="RN" pin="4" pad="7"/>
<connect gate="RN" pin="5" pad="8"/>
<connect gate="RN" pin="6" pad="6"/>
<connect gate="RN" pin="7" pad="4"/>
<connect gate="RN" pin="8" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MM58174" prefix="U">
<gates>
<gate name="G$1" symbol="MM58174"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="!CS" pad="1"/>
<connect gate="G$1" pin="!INT" pad="13"/>
<connect gate="G$1" pin="!RD" pad="2"/>
<connect gate="G$1" pin="!WR" pad="3"/>
<connect gate="G$1" pin="AD0" pad="12"/>
<connect gate="G$1" pin="AD1" pad="11"/>
<connect gate="G$1" pin="AD2" pad="10"/>
<connect gate="G$1" pin="AD3" pad="9"/>
<connect gate="G$1" pin="DB0" pad="8"/>
<connect gate="G$1" pin="DB1" pad="6"/>
<connect gate="G$1" pin="DB2" pad="5"/>
<connect gate="G$1" pin="DB3" pad="4"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="7"/>
<connect gate="G$1" pin="XI" pad="15"/>
<connect gate="G$1" pin="XO" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="X2210D" prefix="U">
<gates>
<gate name="G$1" symbol="X2210D"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="!CS" pad="7"/>
<connect gate="G$1" pin="!RECALL" pad="10"/>
<connect gate="G$1" pin="!STORE" pad="9"/>
<connect gate="G$1" pin="!WE" pad="11"/>
<connect gate="G$1" pin="A0" pad="6"/>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="3"/>
<connect gate="G$1" pin="A4" pad="2"/>
<connect gate="G$1" pin="A5" pad="16"/>
<connect gate="G$1" pin="IO1" pad="12"/>
<connect gate="G$1" pin="IO2" pad="13"/>
<connect gate="G$1" pin="IO3" pad="14"/>
<connect gate="G$1" pin="IO4" pad="15"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC1" pad="17"/>
<connect gate="G$1" pin="VDD" pad="18"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*161" prefix="V">
<description>Synchrounus 4-bit &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="161"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CLR" pad="1"/>
<connect gate="1" pin="!LOAD" pad="9"/>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="B" pad="4"/>
<connect gate="1" pin="C" pad="5"/>
<connect gate="1" pin="CLK" pad="2"/>
<connect gate="1" pin="D" pad="6"/>
<connect gate="1" pin="ENP" pad="7"/>
<connect gate="1" pin="ENT" pad="10"/>
<connect gate="1" pin="QA" pad="14"/>
<connect gate="1" pin="QB" pad="13"/>
<connect gate="1" pin="QC" pad="12"/>
<connect gate="1" pin="QD" pad="11"/>
<connect gate="1" pin="RCO" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*163" prefix="V">
<description>Synchrounus 4-bit &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="163"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CLR" pad="1"/>
<connect gate="1" pin="!LOAD" pad="9"/>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="B" pad="4"/>
<connect gate="1" pin="C" pad="5"/>
<connect gate="1" pin="CLK" pad="2"/>
<connect gate="1" pin="D" pad="6"/>
<connect gate="1" pin="ENP" pad="7"/>
<connect gate="1" pin="ENT" pad="10"/>
<connect gate="1" pin="QA" pad="14"/>
<connect gate="1" pin="QB" pad="13"/>
<connect gate="1" pin="QC" pad="12"/>
<connect gate="1" pin="QD" pad="11"/>
<connect gate="1" pin="RCO" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PAD-N" prefix="X" uservalue="yes">
<description>&lt;b&gt;PAD SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PAD-N"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8274" prefix="U">
<gates>
<gate name="G$1" symbol="8274"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!CDA" pad="3"/>
<connect gate="G$1" pin="!CDB" pad="5"/>
<connect gate="G$1" pin="!CS" pad="23"/>
<connect gate="G$1" pin="!CTSA" pad="39"/>
<connect gate="G$1" pin="!CTSB" pad="6"/>
<connect gate="G$1" pin="!DRTA" pad="31"/>
<connect gate="G$1" pin="!DRTB" pad="26"/>
<connect gate="G$1" pin="!INT" pad="28"/>
<connect gate="G$1" pin="!INTA" pad="27"/>
<connect gate="G$1" pin="!RD" pad="22"/>
<connect gate="G$1" pin="!RESET" pad="2"/>
<connect gate="G$1" pin="!RTSA" pad="38"/>
<connect gate="G$1" pin="!RXCA" pad="35"/>
<connect gate="G$1" pin="!RXCB" pad="4"/>
<connect gate="G$1" pin="!SYNDETA" pad="33"/>
<connect gate="G$1" pin="!SYNDETB/RTSB" pad="10"/>
<connect gate="G$1" pin="!TXCA" pad="36"/>
<connect gate="G$1" pin="!TXCB" pad="7"/>
<connect gate="G$1" pin="!WR" pad="21"/>
<connect gate="G$1" pin="A0" pad="25"/>
<connect gate="G$1" pin="A1" pad="24"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="D0" pad="19"/>
<connect gate="G$1" pin="D1" pad="18"/>
<connect gate="G$1" pin="D2" pad="17"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="15"/>
<connect gate="G$1" pin="D5" pad="14"/>
<connect gate="G$1" pin="D6" pad="13"/>
<connect gate="G$1" pin="D7" pad="12"/>
<connect gate="G$1" pin="RDYA/RXDRQA" pad="32"/>
<connect gate="G$1" pin="RDYB/TXDRQA" pad="11"/>
<connect gate="G$1" pin="RXDA" pad="34"/>
<connect gate="G$1" pin="RXDB" pad="9"/>
<connect gate="G$1" pin="TRXDRQB/!IPI" pad="29"/>
<connect gate="G$1" pin="TXDA" pad="37"/>
<connect gate="G$1" pin="TXDB" pad="8"/>
<connect gate="G$1" pin="TXDRQB/!IPO" pad="30"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X5" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X5"/>
</gates>
<devices>
<device name="" package="2X05">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X05/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X12" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X12"/>
</gates>
<devices>
<device name="" package="2X12">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X12/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="21" pad="21"/>
<connect gate="A" pin="22" pad="22"/>
<connect gate="A" pin="23" pad="23"/>
<connect gate="A" pin="24" pad="24"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X17" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINH2X17"/>
</gates>
<devices>
<device name="" package="2X17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X17/90">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X10" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X10"/>
</gates>
<devices>
<device name="" package="2X10">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="/90" package="2X10/90">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="10" pad="10"/>
<connect gate="A" pin="11" pad="11"/>
<connect gate="A" pin="12" pad="12"/>
<connect gate="A" pin="13" pad="13"/>
<connect gate="A" pin="14" pad="14"/>
<connect gate="A" pin="15" pad="15"/>
<connect gate="A" pin="16" pad="16"/>
<connect gate="A" pin="17" pad="17"/>
<connect gate="A" pin="18" pad="18"/>
<connect gate="A" pin="19" pad="19"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="20" pad="20"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
<connect gate="A" pin="7" pad="7"/>
<connect gate="A" pin="8" pad="8"/>
<connect gate="A" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4194" prefix="U">
<gates>
<gate name="G" symbol="4194"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G" pin="BAL" pad="4"/>
<connect gate="G" pin="COMP+" pad="3"/>
<connect gate="G" pin="COMP-" pad="5"/>
<connect gate="G" pin="GND" pad="12"/>
<connect gate="G" pin="NC" pad="2 6 9 13"/>
<connect gate="G" pin="RO" pad="10"/>
<connect gate="G" pin="RSET" pad="11"/>
<connect gate="G" pin="VIN+" pad="14"/>
<connect gate="G" pin="VIN-" pad="7"/>
<connect gate="G" pin="VO+" pad="1"/>
<connect gate="G" pin="VO-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC3488" prefix="U">
<gates>
<gate name="G$1" symbol="MC3488"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="!OUTA" pad="7"/>
<connect gate="G$1" pin="!OUTB" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="INA" pad="2"/>
<connect gate="G$1" pin="INB" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VEE" pad="5"/>
<connect gate="G$1" pin="WS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*06" prefix="IC">
<description>Hex &lt;b&gt;INVERTER&lt;/b&gt;, open collector high-voltage output</description>
<gates>
<gate name="A" symbol="7405"/>
<gate name="B" symbol="7405"/>
<gate name="C" symbol="7405"/>
<gate name="D" symbol="7405"/>
<gate name="E" symbol="7405"/>
<gate name="F" symbol="7405"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I" pad="4"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I" pad="8"/>
<connect gate="C" pin="O" pad="9"/>
<connect gate="D" pin="I" pad="13"/>
<connect gate="D" pin="O" pad="12"/>
<connect gate="E" pin="I" pad="16"/>
<connect gate="E" pin="O" pad="14"/>
<connect gate="F" pin="I" pad="19"/>
<connect gate="F" pin="O" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*14" prefix="IC">
<description>Hex schmitt trigger &lt;b&gt;INVERTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7414"/>
<gate name="B" symbol="7414"/>
<gate name="C" symbol="7414"/>
<gate name="D" symbol="7414"/>
<gate name="E" symbol="7414"/>
<gate name="F" symbol="7414"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I" pad="11"/>
<connect gate="B" pin="O" pad="10"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I" pad="1"/>
<connect gate="D" pin="O" pad="2"/>
<connect gate="E" pin="I" pad="3"/>
<connect gate="E" pin="O" pad="4"/>
<connect gate="F" pin="I" pad="5"/>
<connect gate="F" pin="O" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I" pad="11"/>
<connect gate="B" pin="O" pad="10"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I" pad="1"/>
<connect gate="D" pin="O" pad="2"/>
<connect gate="E" pin="I" pad="3"/>
<connect gate="E" pin="O" pad="4"/>
<connect gate="F" pin="I" pad="5"/>
<connect gate="F" pin="O" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I" pad="4"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I" pad="8"/>
<connect gate="C" pin="O" pad="9"/>
<connect gate="D" pin="I" pad="13"/>
<connect gate="D" pin="O" pad="12"/>
<connect gate="E" pin="I" pad="16"/>
<connect gate="E" pin="O" pad="14"/>
<connect gate="F" pin="I" pad="19"/>
<connect gate="F" pin="O" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*259" prefix="IC">
<description>8-bit addressable &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74259"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="CLR" pad="15"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="G" pad="14"/>
<connect gate="A" pin="Q0" pad="4"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="6"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="Q5" pad="10"/>
<connect gate="A" pin="Q6" pad="11"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="3"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="CLR" pad="15"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="G" pad="14"/>
<connect gate="A" pin="Q0" pad="4"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="6"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="Q5" pad="10"/>
<connect gate="A" pin="Q6" pad="11"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="3"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="16L8" prefix="IC" uservalue="yes">
<description>&lt;b&gt;PAL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="16L8"/>
<gate name="P" symbol="PWRN-2"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="I0" pad="1"/>
<connect gate="G$1" pin="I1" pad="2"/>
<connect gate="G$1" pin="I2" pad="3"/>
<connect gate="G$1" pin="I3" pad="4"/>
<connect gate="G$1" pin="I4" pad="5"/>
<connect gate="G$1" pin="I5" pad="6"/>
<connect gate="G$1" pin="I6" pad="7"/>
<connect gate="G$1" pin="I7" pad="8"/>
<connect gate="G$1" pin="I8" pad="9"/>
<connect gate="G$1" pin="I9" pad="11"/>
<connect gate="G$1" pin="O0" pad="12"/>
<connect gate="G$1" pin="O1" pad="13"/>
<connect gate="G$1" pin="O2" pad="14"/>
<connect gate="G$1" pin="O3" pad="15"/>
<connect gate="G$1" pin="O4" pad="16"/>
<connect gate="G$1" pin="O5" pad="17"/>
<connect gate="G$1" pin="O6" pad="18"/>
<connect gate="G$1" pin="O7" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TIBPAL16L8-7CN"/>
<attribute name="OC_FARNELL" value="1510033"/>
<attribute name="OC_NEWARK" value="08F8522"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XO-" prefix="QG" uservalue="yes">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="QG3"/>
</gates>
<devices>
<device name="8" package="DIL08S">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="TS" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="14" package="DIL14S">
<connects>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="TS" pad="1"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
